For 1990-2009 cars

### Removal Procedure

Notice: When removing body panels, apply tape to corners of panel and adjacent surfaces to help prevent paint damage.

1. Raise the hood.
2. Install a protective covering over the fenders in order to prevent damage to the paint.
3. Remove the hood hinge pivot bolts.
4. With the help of an assistant, remove the hood.

### Installation Procedure

1. Install the hood.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the hood hinge pivot bolts.

Tighten
Tighten the hood hinge pivot bolts to 17 N·m (13 lb ft).

3. Align the hood. Refer to Hood Adjustment .