For 1990-2009 cars

### Removal Procedure

1. Remove the lower window to full down position.
2. Remove the door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
3. Remove the door window frame applique. Refer to Front Door Frame Applique Replacement .
4. Remove the outside mirror. Refer to Outside Rearview Mirror Replacement .
5. Disengage the door upper auxiliary sealing strip fasteners (3).
6. Disengage the door upper auxiliary sealing strip from the door frame (1).

### Installation Procedure

1. Engage the door upper auxiliary sealing strip to the door frame (1).
2. Engage the door upper auxiliary sealing strip fasteners.
3. Install the outside mirror. Refer to Refer to Outside Rearview Mirror Replacement .
4. Install the door window frame applique. Refer to Front Door Frame Applique Replacement .
5. Install the door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .