For 1990-2009 cars

### Removal Procedure

1. Loosen the clamp on the air cleaner outlet duct .
2. Remove the air cleaner outlet duct from the air cleaner outlet resonator.
3. Remove the mounting screw from the air cleaner outlet resonator.
4. Disconnect the clamp from the air cleaner outlet resonator at the throttle body.
5. Raise the air cleaner outlet resonator from the throttle body.
6. Disconnect the crankcase vent hose from the air cleaner outlet resonator.
7. Remove the air cleaner outlet resonator.

### Installation Procedure

1. Install the crankcase vent hose to the air cleaner outlet resonator.

Important: Be sure the air cleaner outlet resonator seals to the throttle body.

2. Install the air cleaner outlet resonator to the throttle body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the mounting screws to the air cleaner outlet resonator .

Tighten
Tighten the mounting screws to 10 N·m (88 lb in).

4. Tighten the clamp on the air cleaner outlet resonator at the throttle body.

Tighten
Tighten the clamp to 5 N·m (44 lb in).

5. Install the air cleaner outlet duct to the air cleaner outlet resonator.
6. Tighten the clamp on the air cleaner outlet duct .

Tighten
Tighten the clamp to 5 N·m (44 lb in).