For 1990-2009 cars

### Removal Procedure

1. Turn the ignition switch to the ACCY position.
2. Set the wiper switch to the PULSE position.
3. Turn the ignition off when the wipers are in the innerwipe position and not moving.
4. Remove the wiper blade assembly from the wiper arm assembly.

4.1. | Push in the button of the wiper blade assembly clip and remove the wiper blade assembly from the inside radius of the wiper arm assembly.

4.2. | Bring the wiper arm assembly out through the opening in the wiper blade assembly.

### Installation Procedure

1. Install the wiper blade assembly onto the wiper arm assembly.
2. Operate the wipers and check for proper operation.