For 1990-2009 cars

#### Tools Required

• | J 36513 Gear and Bearing Separator Plate

• | J 44378 Press Adapter (all shafts)

Important: The 4th driven gear is a very tight press.

1. Press off the 4th driven gear using the J 36513 (2) and the J 44378 (1).

Important: The 3rd driven gear is a very tight press.

2. Remove the 3rd driven gear using the J 36513 (2) and the J 44378 (1).
3. Remove the 5th gear (1) and the two caged needle bearings (2).

Important: Do not contact the thrust washer under the reverse gear.

4. Remove the bearing collar using the J 36513 (2), under the reverse gear, the J 44378 (1), and a hydraulic press.
5. Remove the following components as an assembly:

5.1. | The bearing collar (1)

5.2. | The 5th gear blocking ring (2)

5.3. | The 5th/Reverse synchronizer assembly (3)

5.4. | The reverse blocking ring (4)

5.5. | The reverse gear (5)

5.6. | The caged needle bearing (6)

Important: Ensure that the J 36513 is not making contact with the pinion gear before pressing off the collar and thrust washer.

6. Remove the collar and the thrust washer using the J 44378 (1), the J 36513 (2), and a hydraulic press.