For 1990-2009 cars

1. Visually inspect the drum brake system hold-down springs (4) for the following:

• | Excessive corrosion

• | Damaged or bent locating pins

• | Broken spring coils

• | Damaged retaining cups

2. Visually inspect the lower return spring (7) and the upper return/adjuster actuator spring (3) for the following:

• | Excessive corrosion

• | Excessive stretching

• | Broken hook ends

• | Twisting or binding

3. If any of the conditions listed were found, the drum brake system hardware requires replacement.
4. Visually inspect the park brake lever (5) for the following:

• | Bent

• | Broken pivot

• | Broken at park brake cable attachment

5. If any of the conditions listed were found, the park brake lever and/or attaching hardware requires replacement.