For 1990-2009 cars

### Removal Procedure

Place window in halfway down position.

1. Remove the run channel weather-strip from the window (1). Refer to Window Channel Replacement .
2. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the water reflector. Refer to Front Side Door Water Deflector Replacement .
4. Remove the bolts which retain the window to the window regulator.
5. Remove the window (1).

### Installation Procedure

1. Install the front window (1).
2. Install the bolts which retain the window to the window regulator.
3. Install the water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .
5. Install the run channel weather strip to the window (1). Refer to Window Channel Replacement .