For 1990-2009 cars

### Removal Procedure

1. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
2. Disconnect the front door window regulator electrical connector.
3. Press the front door window motor retaining tabs (1) out to release the front door window regulator motor from the front door system locking module.
4. Remove the front door window regulator from the front door system locking module.

### Installation Procedure

1. Position the front door window regulator motor to the alignment pins on the front door locking system module.
2. Press the front door window regulator motor onto the front door locking system module until the retaining tabs (1) are fully seated over the front door window regulator motor ends.
3. Connect the front door window regulator motor electrical connector.
4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .