For 1990-2009 cars

#### Tools Required

Cigarette Lighter Socket Remover

### Removal Procedure

1. Remove the 12 volt power supply fuse.
2. Remove the 12 volt power supply socket by placing one side of the "T" portion of the tool into the tab window and then the other should be angled into the opposite tab window, then pull the 12 volt power supply socket straight out.
3. Remove the tool from the 12 volt power supply socket.
4. Disconnect the electrical connector from the instrument panel 12 volt power supply.
5. Remove the 12 volt power supply retainer using your index finger and pulling out.

### Installation Procedure

1. Position the 12 volt power supply retainer with the key to the slot into the 12 volt power supply hole.
2. Install the 12 volt power supply retainer pressing into place until fully seated.
3. Connect the electrical connector to the instrument panel 12 volt power supply.
4. Position the 12 volt power supply to the retainer.
5. Install the 12 volt power supply into the instrument panel pressing into place until fully seated.
6. Install the 12 volt power supply fuse.
7. Inspect the 12 volt power supply for proper operation.