For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 9886-01 Door Handle Clip Remover

1. Remove the spring clip by inserting the J 9886-01 between the window regulator handle and the door window regulator handle bearing plate.
2. Push the door window regulator handle (2) inward in order to remove the handle.
3. Remove the door window regulator handle bearing plate (1).

### Installation Procedure

1. Place window in halfway down position.
2. Raise the window to the full up position.
3. Install the clip to the door window regulator handle (2).
4. Install the door window regulator handle bearing plate (1).
5. Position the door window regulator handle.
6. Push the door window regulator handle in order to secure the handle.