For 1990-2009 cars

## Front Fog Lamp Replacement Pontiac

### Removal Procedure

Caution: Halogen bulbs contain gas under pressure. Handling a bulb improperly could cause it to shatter into flying glass fragments. To help avoid personal injury:

• | Turn off the lamp switch and allow the bulb to cool before changing the bulb.

• | Leave the lamp switch OFF until the bulb change is complete.

• | Always wear eye protection when changing a halogen bulb.

• | Handle the bulb only by its base. Avoid touching the glass.

• | Keep dirt and moisture off the bulb.

• | Properly dispose of the used bulb.

• | Keep halogen bulbs out of the reach of children.

1. Partially remove the front edge of the front fender liner in order to gain access to the fog lamps. Refer to Front Fender Liner Replacement in Body Front End.
2. Remove the bulb/socket from the fog lamp by rotating counterclockwise.
3. Disconnect the electrical connector from the bulb/socket, if required.
4. Remove the bolts from the fog lamp.
5. Remove the fog lamp from the front bumper impact bar.

### Installation Procedure

1. Position the fog lamp to the front bumper impact bar.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the fog lamp bolts to the fog lamp.

Tighten
Tighten the fog lamp bolts to 3 N·m (27 lb in).

3. Connect the electrical connector to the bulb/socket, if required.
4. Install the bulb/socket to the fog lamp.
5. Rotate the bulb/socket clockwise to secure it to the fog lamp.
6. Check and adjust the fog lamp aim, if required. Refer to Fog Lamp Aiming .
7. Install the front edge of the front fender liner. Refer to Front Fender Liner Replacement in Body Front End.

## Front Fog Lamp Replacement Oldsmobile

### Removal Procedure

Caution: Halogen bulbs contain gas under pressure. Handling a bulb improperly could cause it to shatter into flying glass fragments. To help avoid personal injury:

• | Turn off the lamp switch and allow the bulb to cool before changing the bulb.

• | Leave the lamp switch OFF until the bulb change is complete.

• | Always wear eye protection when changing a halogen bulb.

• | Handle the bulb only by its base. Avoid touching the glass.

• | Keep dirt and moisture off the bulb.

• | Properly dispose of the used bulb.

• | Keep halogen bulbs out of the reach of children.

1. Partially remove the front edge of the front fender liner to gain access to the fog lamps. Refer to Front Fender Liner Replacement in Body Front End.
2. Remove the bulb/socket from the fog lamp by rotating counterclockwise.
3. Disconnect the electrical connector from the bulb/socket, if required.
4. Remove the bolts (1) from the fog lamp.
5. Remove the fog lamp from the front bumper impact bar.

### Installation Procedure

1. Connect the electrical connector to the bulb/socket, if required.
2. Install the bulb/socket to the fog lamp.
3. Rotate the fog lamp bulb/socket clockwise until fully seated.
4. Position the fog lamp to the front bumper impact bar.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the fog lamp bolts (1) to the fog lamp.

Tighten
Tighten the fog lamp bolts to 3 N·m (27 lb in).

6. Check and adjust the fog lamp aim, if necessary. Refer to Fog Lamp Aiming .
7. Install the front edge of the front fender liner. Refer to Front Fender Liner Replacement in Body Front End.