For 1990-2009 cars

1. Remove the fuel return hose and clamp from the fuel injection pump.
2. Remove the fuel injection pump high pressure line from the fuel injection pump.
3. Remove the fuel inlet hose from the fuel injection pump.
4. Remove the fuel inlet distribution block bolt and nut.
5. Remove the fuel inlet distribution block from the fuel return distribution block.
6. Remove the fuel inlet to fuel return line clamp bolt.
7. Remove the fuel inlet to fuel return line clamp.
8. Remove the function block nuts.
9. Remove the fuel inlet pipe assembly.
10. Remove the left fuel rail high pressure line (1).
11. Remove the left cylinder head return line eye bolt and gasket (2).
12. Remove the right fuel rail high pressure line (1).
13. Remove the right cylinder head return line eye bolt and gasket (2).
14. Remove the fuel return line clamp bolt and clamp.
15. Remove the fuel pressure limiting valve bracket nut.
16. Remove the fuel pipes and function block assembly.
17. Remove the anti-rotation locks from the left bank injection pipes.
18. Remove the injection pipes from the left bank.
19. Remove the anti-rotation locks from the right bank injection pipes.
20. Remove the injection pipes from the right bank.
21. Remove the left fuel rail mounting bolts.
22. Remove the left fuel rail.
23. Remove the right fuel rail mounting bolts.
24. Remove the right fuel rail.