For 1990-2009 cars

#### Special Tools

J-38125 Terminal Repair Kit

Use the following repair procedures in order to repair the following:

• | Push to Seat terminals

• | Pull to Seat terminals

Some terminals do not require all of the steps shown. Skip the steps that do not apply for your terminal repair. The J-38125 contains further information.

1. Cut off the terminal between the core and the insulation crimp. Minimize any wire loss.

For cable seal terminals, remove the seal.

2. Apply the correct cable seal per gage size of the wire, if used.

Slide the seal back along the wire in order to enable insulation removal.

3. Remove the insulation.
4. For sealed terminals only, align the seal with the end of the cable insulation.
5. Position the strip in the terminal.

For sealed terminals, position the strip and seal in the terminal.

6. Hand crimp the core wings.
7. Hand crimp the insulation wings.

For sealed terminals, hand crimp the insulation wings around the seal and the cable.

8. Solder all of the hand crimp terminals excepting Micro-Pack 100.64 size. Soldering Micro-Pack 100 World terminals may damage the terminal.