For 1990-2009 cars

### Gasket Reuse and Applying Sealant

• | Do not reuse any gasket unless specified.

• | Gaskets that can be reused will be identified in the service procedure.

• | Do not apply sealant to any gasket or sealing surface unless specified in the service procedure.

### Separating Components

• | Use a rubber mallet in order to separate the components.

• | Bump the part sideways in order to loosen the components.

• | Bumping of the component should be done at bends or reinforced areas of the component to prevent distortion of the components.