For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the rear seat back cushion. Refer to Rear Seat Back Replacement .
3. Remove the rear window panel trim panel. Refer to Rear Window Shelf Trim Panel Replacement .
4. Remove the rear seat belt retractor anchor plate bolt.
5. Remove the rear seat belt retractor bolt (1).
6. Remove the rear seat outer retractor side belt.

### Installation Procedure

Important: Remove any twists in the seat belt webbing before final assembly.

1. Install the rear seat outer retractor side belt.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear seat belt retractor bolt (1).

Tighten
Tighten the rear seat belt retractor bolt to 36 N·m (27 lb ft).

3. Install the rear seat belt retractor anchor plate bolt.

Tighten
Tighten the rear seat belt retractor anchor plate bolt to 42 N·m (31 lb ft).

4. Install the rear window panel trim panel. Refer to Rear Window Shelf Trim Panel Replacement .
5. Install the rear seat cushion. Refer to Rear Seat Back Replacement .
6. Install the rear seat back cushion. Refer to Rear Seat Cushion Replacement .