MODEL PAINT INFORMATION PAINT CODES. Oldsmobile Custom Cruiser 1984

For 1990-2009 cars

# MODEL PAINT INFORMATION PAINT CODES

#### MODEL/YEARS ALL 1984 MODELS

The three production paint suppliers (Ditzler, DuPont and Rinshed-Mason), now have 1984 service paint numbers released. The paints listed in this bulletin will be available from local paint suppliers in the near future.

#### NOTE: Service paint is also available from paint refinish specialists such as Sherwin-Williams, Acme, Rogers, and Martin-Senour. Paint suppliers in your area can provide you with information regarding these materials.

When contacting your local paint supplier for repair materials, make sure that you specify the type of material needed. If your paint supplier is unable to provide you with the material needed, ask him to contact his manufacturer sales representative for assistance.

EXTERIOR COLORS Sherwin- Paint Inmont Williams Martin- Code Color Name Ditzler Dupont (R.M.) (Acme/Rogers) Senour ---- ---------- ------- ------ ------ ------------ ------ 11 White 2058 5338 2080 L10A-2864 30-3929 5644 17 Sliver Met 3659 8536 14072 33956 30-5315 19 Black 9300 99 A946 L10B-1738 3069 3000-4590 22 Lt. Royal Blue Met. 3522 B8308 13106 32895 30-5229 27 Med. Dk. Royal Blue Met 3525 B8304 13110 32701 30-5179 42 Lt. Gray Fern Met. 3526 B8309 13114 32902 30-5234 48 Dk. Gray Fern Met. 3528 B8303 13115 32702 30-5180 59 Pastel Biege 45205 13521 L10H-3902 30-4731 25401 60 Lt. Sand Gray 3530 B8307 13120 32704 30-5182 62 Lt. Briar Brown Met 3531 B8310 13121 32896 30-5230 67 Dk. Briar Brown Met. 3533 B8305 13127 32705 30-5183 73 Lt. Maple Met. B8108 13522V 31055 30-4988 74 Autumn Maple F/M 3532 B8385 13131V 33074 30-5244 75 Spectra Red 3332 B8115 12229V 31056 30-4989 78 Dk Autumn Maple Met. 3553 C8310 13132F 33075 30-5245 85 Saddlle Met. r/M B8468 14073D 33753 30-5293 87 Med Sand Gray F/M 3538 B8311 13135 32706 30-5184

INTERIOR COLORS

#### NOTICE: Ditzler DIA is Duracryl Interior Lacquer, Ditzler UCV is Liquid Vinyl Paint for Vinyl and ABS plastic parts (instrument panels, door trim panels, seats, etc.) DuPont is Interior Lacquer. Rinshed-Mason is Interior Lacquer. Sherwin-Williams is Interior Lacquer. When painting interior flexible parts, add R-M 891 flex agent.

Sherwin- Code Ditzler Ditzler Inmont Williams Martin/ Semi- Color Name DIA UCV Dupont (R.M.) Acme/Rogers Senour Gloss ---------- --- --- ------ ------ ------------ ------ ----- 17 Med. Dk. Charcoal 33569 2-1034 C8339 13195 32841 32-17020 17 Dark Charcoal 33570 2-976 C8387 31394 32842 32-17021 19 Black 9387 120 4428 4401 J4-3960 32-16082 90681 22 Med. Dk. Royal Blue 15680 2-1033 C8334 13192 32999 32-16915 22 Dark Royal Blue 15632 2-974 C8443 13191D 32839 32-17018 42 Med. Grayfern 33586 2-975 C8386 13187D 32840 32-17019 42 Dark Grayfern 33587 2-971 C8444 13186 32836 32-17015 60 Lt. Sand Gray 33567 2-972 C8384 13182 32837 32-17016 60 Med.Sand Gray 33568 2-973 C8329 13181 32838 32-17017 61 Med.Saddle Tan 24997 2-878 D8208 12739 31892 32-16842 61 Dark Saddle Tan 24999 2-880 D8217 12741 31893 32-16843 67 Med.Dk. Briar Brown 25306 2-1043 C8392 13176D 33283 32-16945 67 Dark Briar Brown 25172 2-970 C8383 13175D 32835 32-17014 77 Med. Dk. Maple 72568 2-1044 C8391 13174D 33284 32-16946 77 Dark Maple 72415 2-803 C8115 12271F 31201 32-16777

FLAT

17 Dark Charcoal 33621 2-976 C8387 13257 32939 32-16878 19 Black 9433 120 4428 12812 J4-8677 32-16615 92387 22 Dark Royal Blue 15682 2-974 C8443 13253D 32936 32-16875 42 Med. Grayfern 33619 2-975 13256D 32852 32-17024 42 Dark Grayfern 33620 2-971 C8327 13250 32935 32-16874 60 Lt. Sand Gray 13251 60 Med. Sand Gray 13252 3285 32-17023 61 Med.Saddle Tan 25056 2-878 D8208 13145 31906 32-16856 61 Dark Saddis Tan 25058 2-880 D8217 12719 32091 32-16858 67 Dark Briar Brown 25229 2-970 C8383 13249D 32934 32-16873 77 Dark Maple 72435 2-803 C8115 13258F 31423 32-16803

PAINT STRIPES

NOTICE : Some plants use decals or tape for stripes.

Paint Sherwin- Paint Inmont Martin Williams Code Color Name Ditzler Dupont (R.M.) Senour Acme/Rogers ---- ----------- ------- ------ ------ ------ ----------- 11A White 0847 5338 2080 32-3929 L10A-2864 5644 19A Black 9300 99 A-946 30069 L10B-1738 3000/4590 25A Dk Royal Blue 13282D 32-26699 34101 27A Med. Dark Royal Blue Met D8304 13110 27A Med. Dark Royal Blue 15639 C8393 13282 32-26617 33154 42A Light Grayfern 32018 C8398 13283 32-26621 33158

Sherwin- Paint Inmont Martin Williams Code Color Name Ditzler Dupont (R.M.) Senour Acme/Rogers

55A Gold D8276 9215 14A Lt. Sand Gray 3530 D8307 13120 32-26627 33164 67A Dark Briar Brown 24945 D8328 13274 32-26628 33165 67A Dark Briar Brown Met. - D8305 13127 75A Red 72128 43592 4518R 32-26272 J4-7191 11892 78A Dark Autumn Maple 51127 D8329 13275R 32-26629 33166 78A Dark Autumn Maple Met. - C8310 13132F

#### ENGINE PAINT

#### NOTICE: 1984 Engine paint is available from WDDGM in the following colors in aerosol form:

Color Part Number Size ----- ----------- ---- Gas Engines Black 1052439 11 oz. Diesel Engines Diesel Blue 1052443 11 oz.

#### VINYL ROOF MOLDING COLORS

Sherwin- Paint Inmont Williams Martin- Number Color Name Ditzler Dupont (R.M.) Acme/Rogers Senour ------ ---------- ------- ------ ------ ----------- ------ 11 White 183 5338 12703 J4-5676 32-26185 11510 19 Black 120 99 4416 J4-1990 32-16062 9739 27 Med. Dark Royal Blue Met. 2-954 B8304 13159D 33175 32-26638 42 Lt. Grayfern Met. 2-955 B8309 13160 33186 32-26649 60 Lt. Sand Gray 2-958 B8307 13163 33178 32-26641 67 Dark Briar Brown Met. 2-960 B8305 13165 33176 32-26639 78 Dark Autumn Maple Met. 2-961 B8306 13166D 33177 32-26640 91 Lt. Flax F/M 2-966 C8303 13168 33181 32-26644

#### WHEEL COLORS

#### NOTICE: Wheels are painted with enamel therefore, please specify this type paint when ordering. Sherwin- Paint Code Inmont Williams Semi-Gloss Color Name Dupont (R.M.) Acme/Rogers Martin-Senour ----------- ---------- ------ ------ ------------ ------------- 11 White 5338 2080 L10A-2864 30-3929 5644 17 Silver Met 33596 30-5315 19 Black 99 A946 L10B-1738 3069 3000/4590 22 Lt. Royal Blue Met B8308 13106 32895 30-5229 27 Med. Dark Royal Blue Met B8304 13110 32701 30-5179 42 Lt. Grayfern Met. B8309 13114 32902 30-5234 48 Dk. Grayfern Met. B8303 13115 32702 30-5180 59 Pastel Beige 1352l L10H-3902 30-4731 25401 60 Lt.Sand Gray B8307 13120 32704 30-5182 62 Lt. Briar Brown Met. B8310 13121 32896 30-5230 67 Dark Briar Brown Met. B8305 13127 32705 30-5183 73 Lt. Maple Met. 13522V 31055 30-4988 75 Spectra Red B8115 12229V 31056 30-4989 78 Dark Autumn Maple Met. C8310 13132F 33075 30-5245 85 Saddle Met. F/M B8468 14073D 33753 30-5293

1984 EXTERIOR PLASTIC PARTS

All 1984 Oldsmobiles have exterior parts made of various types of plastic materials that require specific procedures to obtain high quality refinishing results. Included in this bulletin is a chart listing the different exterior parts and the type of plastic materials used on 1984 models. For best results when painting is required, determine the type of plastic material from the chart; then follow the correct paint procedure, depending upon what painting material and equipment is available.

PART NAME PLASTIC TYPE SYMBOL --------- ------------- ------- FIRENZA Front Fasica Thermoset Urethane RRIM Rear Fasica Thermoset Urethane RRIM

OMEGA MODELS

Lower Valance Panel, Front (1 pc.) Thermoplastic Uretharn TPU Front End Panel, (1 pc.) Thermosetting Polyester UP Rear Bumper Fillers (5 pc.) Thermoplastic Urethane TPU Lower Valance Panel, Rear Thermoplastic Urethane TPU Front Bumper Fascia (W48) Thermoplastic Urethane RIM Front End Panel Thermoset Urethane RRIM

CUTLASS CIERA - CUTLASS SUPREME

*Front Bumper Outer Fillers R&L (2 pcs.) Thermoplastic Elastomer TPE *Front Bumper to Fender R & L (2 pcs.) Thermoplastic Elastomer TPE Front End Panel (1 pc.) Thermosetting Polyester UP *Rear Center Filler (1 pc.) Thermoplastic Elastomer TPE *Rear Bumper Fillers Outers (2 pcs.) Thermoplastic Elastomer TPE *Rear Body to Bumper Filler (2 pcs.) Thermoplastic Elastomer TPE Front Fasica Thermoset Urethane RRIM Rear Fasica Thermoset Urethene RRIM

*Cutlass Supreme Models Only

88 MODELS

Front Bumper to Fender R & L (2 pcs.) Thermoplastic Elastomer TPE Front Bumper Filler, Outers (2 pcs.) Thermoplastic Elastomer TPE Front End Panel (1 pc.) Thermosetting Polyester UP Rear Bumper Fillers (2 pcs.) Thermoplastic Urethane TPU Rear Center Bumper Filler (1 pc.) Thermoplastic Elastomer TPE Rear Bumper Fillers (3 pcs.) Thermoplastic Elastomer TPE (Wagon Only)

98 MODELS

Front Bumper to Fender R & L (2 pcs.) Thermoplastic Elastomer TPE Front Bumper Filler, Outer (2 pcs.) Thermoplastic Elastomer TPE Front End Panel (1 pc.) Thermosetting Polyester UP Rear Bumper Fillers (2 pcs.) Thermoplastic Urethans TPU Rear Center Bumper Filler Thermoplastic Elastomer TPE

TORONADO MODELS

Front Bumpers Filler, Center (1 pc.) Thermoplastic Elastomer TPE Front Bumper Filler, Outers (2 pcs.) Thermoplastic Elastomer TPE Rear Bumper Filler, Center (1 pc.) Thermoplastic Elastomer TPE Rear Bumper Filler, Outers (2 pcs.) Thermoplastic Urethane TPU Front End Panel (1 pc.) Thermosetting Polyester UP

I. General Paint Procedure for Exterior Flexible Plastics

Polyvinylchloride (PVC), Polyurethane (PUR, TPUR, RRIM, RIM) Thermoplastic Elastomer (TPE), EPDM Rubber (Supplied in Prime).

There is a multitude of finishing systems available on the market for painting and/or repairing flexible plastic parts. Following is a general outline of painting procedures including a list of available products. Refer to the manufacturer's literature available through their jobbers for details on proper mixing and application.

A. Thoroughly clean part by washing with a suitable cleaning solvent to remove all surface contaminates.

#### NOTE: Previously painted parts that show signs of cracking, peeling or improper adhesion must be stripped before repainting. The old finish may be removed with any commercially available chlorinated solvent stripper or lacquer thinner.

#### NOTICE: Do not soak parts longer than necessary to remove the old paint to avoid swelling.

B. Scuff sand to an even dull appearance the entire surface to be painted with fine (400 grit or less) sandpaper and feather edge any damaged areas and rewash as in Step A above.

#### NOTE: Unpainted parts do not require sanding prior to painting but should be thoroughly cleaned as in Step A above.

C. Apply two (2) thin coats of primer when required per top coat manufacturer's recommendation and allow to completely dry before proceeding (for most products, approximately 30 minutes)

D. Prepare color coat according to the manufacturer's recommendation and apply sufficient double coats to develop the proper shade. For best results allow a few minutes flash time between each double coat and allow to completely dry before using.

E. Following is a list of some of the products available for painting flexible plastic.

Ditzler Elastometic Primer - DPX844 Ditzler Flexative - DX369 (Permanent Flexible Urethane Additive) Ditzler Flex Additive - DX1798 (Non-Urethane Additive) Ditzler Delthane - DXR80 (Acryic Enamel Hardner) Rinshed-Mason Acrylic Flex Agent 891 DuPont Dexlar Flexible Finish (Lucite tints plus Dexlar 365B Additive) Sherwin-Williams Flex Additive - V2V297 Acme/Rogers Flex Additive - 699/4699 Martin-Senour Flex Additive - 3082

*Cleaning Solvents

1. DuPont Prep-Sol

2. Rinshed-Mason Pre-kleano 900

3. Ditzler Acryli-Clean DX330

4. Sherwin-Williams R7K156

5. Acme 88; Rogers 088

6. Martin-Senour 6383

II. NYLON - will be supplied in prime. Use the same procedure to refinish as on sheet metal parts.

III. ACRYLONNITRILE-BUTADIENE-STYRENE (ABS) -- No prime required, paint with acrylic lacquer.

IV. POLYESTER PARTS (UP, PBTP) - will be supplied in prime and/or black paint. Use the same procedure to refinish or repair as on sheet metal parts.

V. POLYPROPYLENE - Interior parts.

A. Wash surface thoroughly with enamel reducer (do not use wax and grease removers)

B. Apply primer immediately and allow to dry completely before color coating.

C. Color coat with lacquer or enamel reduced and applied according to the manufacturers recommendation.

D. Materials

Cleaning Solvent - DuPont 3812S Enamel Reducer

Ditzler DTE-101 or DTE-102 "Bobcat" enamel reducer

Primer - DuPont 3293 GM 1052364

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.