FRONT DOOR WILL NOT STAY OPEN ON A SLIGHT INCLINE-NEW SPRING. Oldsmobile Custom Cruiser 1991

For 1990-2009 cars

# FRONT DOOR WILL NOT STAY OPEN ON A SLIGHT INCLINE-NEW SPRING

#### SUBJECT: FRONT DOORS WON'T HOLD OPEN ON AN INCLINE OR ARE OR ARE HARD TO OPEN, REPLACE HOLD OPEN SPRING

#### MODELS/YEARS: 1991 CUSTOM CRUISER

CONDITION: Front doors won't hold open on a slight incline or front doors are hard to open.

CAUSE: Door hold open spring is too weak or too strong on vehicles prior to vehicle number MW302803.

CORRECTION: Replace the door hold open spring with P/N 20361482. Be sure to replace both RH and LH front door hold open springs at the time of repair. Parts are currently available from GMSPO.

SPRING REMOVAL TOOL: A loaner tool program has been set up through Kent-Moore. Just call 1-800-345-2233 and ask for J-39079-LNR. Due to the limited number of tools available, please schedule vehicles in a timely manner and return the loan tool as soon as possible using the return label.

#### WARRANTY INFORMATION:

Labor Operation Number: B4050 (Right) B4051 (Left) Labor Time: 0.2 hour per side Add: 0. 1 hour (to paint) Material Allowance: GA in Laquer Chart or $1.98 Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.