PAINT INFORMATION EXTERIOR AND INTERIOR CODES. Oldsmobile Custom Cruiser 1986

For 1990-2009 cars

# PAINT INFORMATION EXTERIOR AND INTERIOR CODES

The three production paint suppliers (Ditzler, DuPont and Rinshed-Mason), now have 1986 service paint numbers released. The paint numbers listed in this bulletin, along with clearcoat materials, are (or soon will be) available from local paint suppliers.

#### NOTICE: Service paint is also available from paint refinish specialists such as Sherwin-Williams, Acme, Rogers, and Martin-Senour. Paint suppliers in your area can provide you with information regarding these materials.

When contacting your local paint supplier for repair materials, make sure that you specify the type of material needed. If your paint supplier is unable to provide you with the material needed, ask supplier to contact the manufacturer's sales representative for assistance.

EXTERIOR PAINT CODES

Paint Color W Inmont Code Name Code Ditzler Dupont (R.M.)

11 White 3967 2058 5338 2080

12 Silver Met. 8535 3746 B8501 15001 13 Silver Met. A/C 9021 3822 D8590 15390 15 Med. Gray Met. 8573 3749 B8502 15004 17 Black Met. C/C 8523 3752 B8537 15007G 19 Black 848 9300 99 A946

22 Lt. Blue Met. C/C 8533 3753 B8538 15008F 24 Bright Blue Met. 8928 3883 B8601 16002 25 Lt. Blue Met. 8574 3754 B8503 15009 27 Med. Blue Met. C/C 8532 3756 B8539 15048V 29 Dk. Blue Met. C/C 8540 3757 B8547 15011D 31 Dark Blue Met. 8592 3760 B8504 15014 40 White C/C 8554 3680 B8469 13570 41 Black C/C 8555 9700 995 13572 42 Lt. Sage Met. C/C 8521 3761 B8540 15015G 43 Lt. Sage Met 8572 3762 B8505 15016 48 Black Emerald Met. C/C 8747 3888 B8608 16006 49 Dk. Sage Met. C/C 8612 3765 B8541 15019F 52 Sedona Tan C/C 8528 3768 B8542 15022 54 Yellow Beige 8525 3769 B8521 15023 58 Lt. Chestnut Met. 8575 3772 B8507 15026 61 Lt. Chestnut Met. C/C 8566 3775 B8543 15029G 62 Dk. Chestnut Met. 8593 3776 B8508 15030 63 Lt. Driftwood C/C 8744 3894 B8603 16011 64 Dk. Chestnut Met. C/C 8567 3777 B8544 15031 65 Lt. R usset Met 8546 3778 B8511 15032V 70 Carmine 8530 3781 B8512 15035V 71 Sparkling Claret Met. 8772 3899 B8602 16016D 74 Flame Red Met C/C 8748 3823 B8610 16017 75 Garnet Red Met. C/C 8746 3900 B8606 16018 78 Dk. Carmine Met C/C 8756 3901 B8624 16019 79 Dk. Red Met. 8529 3786 B8509 15040M 84 Gun Metal Met C/C 7782 3667 B8403 14066D 90 White Diamond C/C 8933 3903 B8609 16021 92 Med. Emeraid F/M C/C 8931 3904 B8607 16022G 94 Med. Blue F/M C/C 8545 3792 B8549 15046D 96 Dk. Driftwood F/M C/C 8765 3906 B8605 16024G 99 Black Cherry Met C/C 8244 3673 B8414 14071D

Paint Color W Sherwin-Williams Code Name Code (Acme/Rogers) Martin-Senour

11 White 3967 LlOA-2864 30-3929 5644 12 Silver Met. 8535 34380 30-5371 13 Silver Met. A/C 9021 35369 30-5491 15 Med. Gray Met. 8573 34381 30-5372 17 Black Met. C/C 8523 34421 30-5409 19 Black 848 LlOB-1738 3069 30001 /4590 22 Lt. Blue Met. C/C 8533 34383 30-5374 24 Bright Blue Met. 8928 35252 30-5471 25 Lt. Blue Met. 8574 34382 30-5373 27 Med. Blue Met. C/C 8532 34384 30-5375 29 Dk. Blue Met. C/C 8540 34385 30-5376 31 Dark Blue Met. 8592 34875 30-5441 40 White C/C 8554 33755 30-5245 41 Black C/C 8555 33756 30-5296 42 Lt. Sage Met. C/C 8521 34387 30-5378 43 Lt. Sage Met 8572 34386 30-5377 48 Black Emerald Met. C/C 8747 35315 30-5482 49 Dk. Sage Met. C/C 8612 34390 30-5381 52 Sedona Tan C/C 8528 34392 30-5383 54 Yellow Beige 8525 34861 30-5437 58 Lt. Chestnut Met. 8575 34396 30-5387 61 Lt. Chestnut Met. C/C 8566 34397 30-5388 62 Dk. Chestnut Met. 8593 34398 30-5389 63 Lt. Driftwood C/C 8744 35310 30-5481 64 Dk. Chestnut Met. C/C 8567 34399 30-5390 65 Lt. R usset Met 8546 34400 30-5391 70 Carmine 8530 34401 30-5392 71 Sparkling Claret Met. 8772 35319 30-5484 74 Flame Red Met C/C 8748 35320 30-5485 75 Garnet Red Met. C/C 8746 35278 30-5477 78 Dk. Carmine Met C/C 8756 35321 30-5526 79 Dk. Red Met. 8529 34405 30-5396 84 Gun Metal Met C/C 7782 33936 30-5313 90 White Diamond C/C 8933 35424 30-5528 92 Med. Emeraid F/M C/C 8931 35255 30-5474 94 Med. Blue F/M C/C 8545 34411 30-5402 96 Dk. Driftwood F/M C/C 8765 35324 30-5486 99 Black Cherry Met C/C 8244 33941 30-5337

#### NOTE: C/C = Basecoat/Clearcoat F/M = Fire Mist.

#### NOTE: Wheels are painted with enamel; therefore, specify this type of paint along with the correct paint code from the exterior color chart when ordering.

INTERIOR COLORS

#### NOTICE: Ditzler DIA is Duracryl Interior Lacquer. Ditzler UCV is Liquid Vinyl Paint for vinyl and ABS plastic parts (instrument panels, door trim panels, seats, etc.) DuPont is Interior Lacquer. Rinshed-Mason is interior Lacquer. Sherwin-Williams is Interior Lacquer. When painting interior flexible parts, add R-M 891 flex agent. When ordering interior paint, be sure to specify whether flat or semi-gloss finish is desired.

Paint W Ditzler Ditzler Inmont Code Code Color Name DIA UVC DuPont (R.M.)

SEMI-GLOSS 19N 48 Black 9433 120 C8535 4402 26BN 594 Med. Blue 15941 - C8546 - 27CN 576 Dk. Blue 15886 2-1098 C8439 15080D 43AN 787 LtSage - - - 43BN 578 Med. Sage 45846 2-1100 D8533 15086 43CN 583 Dk. Sage 45839 2-1118 C8552 - 48BN 796 Med. Emerald 4589 2-1165 * 16059 48DN 788 Dk. Emerald 45890 2-1166 * - 48EN 324 Very Dk.Em. 45932 2-1167 * - 49DN 581 Midnight Sage Gr. - - * 15082G 60AN 782 Lt. Driftwood 25644 2-1169 * 16056 6OBN 802 Med. Driftwood 25778 2-1178 * - 6OCN 790 Dk. Driftwood 25648 2-1170 * - 62AN 769 Lt. Saddle 25230 2-1025 C8352 13180 62BN 806 Med. Saddle 25231 2-1026 * - 62CN 613 Dk. Saddle 25503 2-1126 C8551 - 62DN 257 Dk. Saddle 25254 2-1086 * - 72DN 8833 Very Dk. Carm. 72800 2-1172 * - 79CN 4887 Claret 51170 2-479 C8537 8763 828N 8656 Med. Slate Gray 33823 - C8547 - 82CN 8247 Med. Dk. Gray 33665 2-1048 C8447 14009 82DN 8595 Dk. Gray 33824 2-1125 C8550 - 99DN 8249 Black Cherry 72575 2-1049 * 14010M

*Not available at this time.

Paint W Sherwin-Williams Code Code Color Name Acme/Rogers Martin/Senour

SEMI-GLOSS 19N 48 Black 33024 32-16918 26BN 594 Med. Blue - - 27CN 576 Dk. Blue 34598 32-17067 43AN 787 LtSage 35009 32-17123 43BN 578 Med. Sage 34809 32-17102 43CN 583 Dk. Sage 34811 32-17103 48BN 796 Med. Emerald 35430 32-17131 48DN 788 Dk. Emerald 35470 32-17149 48EN 324 Very Dk.Em. 35543 32-17161 49DN 581 Midnight Sage Gr. - - 60AN 782 Lt. Driftwood 35428 32-17129 6OBN 802 Med. Driftwood 35431 32-17132 6OCN 790 Dk. Driftwood 35471 32-17150 62AN 769 Lt. Saddle 32996 32-16912 62BN 806 Med. Saddle 35469 32-17148 62CN 613 Dk. Saddle 34603 32-17072 62DN 257 Dk. Saddle 33716 32-16951 72DN 8833 Very Dk. Carm. 35544 32-17152 79CN 4887 Claret 34638 32-17084 828N 8656 Med. Slate Gray 34604 32-17073 82CN 8247 Med. Dk. Gray 33714 32-16949 82DN 8595 Dk. Gray 34602 32-17071 99DN 8249 Black Cherry 33791 32-170443

Paint W Ditzler Ditzler Inmont Code Code Color Name DIA UVC DuPont (R.M.)

FLAT 12DN 7701 Graphite - - C8555 - 19N 848 Black - - 4428 -

27CN 8576 Dk. Blue - - C8562 - 43BN 8578 Med. Sage 45879 - D8520 - 43CN 8583 Dk. Sage 45871 - C8567 15093 44DN 7324 Very Dk. Em. - - - 12393 48BN 8796 Med. Emerald - - C8621 - 48DN 8788 Dk. Emerald - - - - 60AN 8782 Lt. Driftwood - - C8623 - 6OBN 8802 Med. Driftwood 25777 - - - 6OCN 8790 Dk. Driftwood - - - 16048 62AN 7769 Lt Saddle - - C8590 - 62BN 8806 Med. Lt. Saddle - - - - 62CN 8613 Dk. Saddle 25570 - C8569 15096 62DN 8257 Dk. Saddle 25581 - - 16044 68CN 8579 Russet - - C8564 - 72CN 8577 Carmine - - C8563 - 72DN 8833 Very Dk. Carm. - - - 16051 79CN 4887 Claret - - C8560 - 82CN 8247 Med. Dk. Gary - - C8556 - 82DN 8595 Dk. Gray - - C8597 15095 99DN 8249 Blk. Cherry - - C8558 -

Paint W Sherwin-Williams Code Code Color Name Acme/Rogers Martin/Senour

12DN 7701 Graphite - - 19N 848 Black J4-8677 32-16615 92387 27CN 8576 Dk. Blue 34606 32-17075 43BN 8578 Med. Sage - - 43CN 8583 Dk. Sage 34610 32-17079 44DN 7324 Very Dk. Em. 31443 32-16806 48BN 8796 Med. Emerald 35439 32-17140 48DN 8788 Dk. Emerald 35436 32-17137 60AN 8782 Lt. Driftwood 35434 32-17135 6OBN 8802 Med. Driftwood 35474 32-17153 6OCN 8790 Dk. Driftwood 35437 32-17138 62AN 7769 Lt Saddle - - 62BN 8806 Med. Lt. Saddle 35545 32-17163 62CN 8613 Dk. Saddle 34612 32-17081 62DN 8257 Dk. Saddle 33773 32-16969 68CN 8579 Russet 34759 32-17087 72CN 8577 Carmine 34607 32-17076 72DN 8833 Very Dk. Carm. 35477 32-17155 79CN 4887 Claret 30814 32-16751 82CN 8247 Med. Dk. Gary 33769 32-16965 82DN 8595 Dk. Gray - - 99DN 8249 Blk. Cherry 33771 32-16967

Paint Stripes

Paint W Inmont Code Code Color Name Ditzler DuPont (R.M.)

11A 3967 White 0847 5338 2080

18A 8291 Gunmetal 33750 C8441 14036 19A 848 Black 9300 99 A946

28A 8659 Dk.Blue 15892 C8521 15074D 43A 8661 Lt.Sage 45842 C8523 15072 45A 8673 Med. Sage 45862 C8532 - 48A 8854 Dk. Emerald Green 45937 C8648 16079 55A 8589 Gold 25509 D8276 15076G 56A 8744 Lt. Driftwood 25802 B8603 16081 58A 8851 Lt. Chestnut 25775 C8641 160831 62A 8660 Lt. Saddle 25551 C8522 - 67A 8001 Dk. Brown 25088 45260 9502

74A 8853 Flame Red 72804 C8642 16085 75A 4721 Red 72128 43592 4518R

76A 8852 Garnet Red 51211 C8643 16086 79A 8663 Dk. Claret 51167 C8525 15071R

Paint W Sherwin-Williams Code Code Color Name (Acme/Rogers) Martin-Senour

11A 3967 White LlOA-2864 32-3929 5644 18A 8291 Gunmetal 34102 32-26700 19A 848 Black LlOB-1738 3069 3000/4590 28A 8659 Dk.Blue 34864 32-26722 43A 8661 Lt.Sage 34866 32-26726 45A 8673 Med. Sage 34872 32-26732 48A 8854 Dk. Emerald Green - - 55A 8589 Gold 34105 32-26703 56A 8744 Lt. Driftwood - - 58A 8851 Lt. Chestnut - - 62A 8660 Lt. Saddle 34865 32-26725 67A 8001 Dk. Brown J4-8727 32-26336 25460 74A 8853 Flame Red - - 75A 4721 Red J4-7191 32-26272 11892 76A 8852 Garnet Red - - 79A 8663 Dk. Claret 34868 32-26705

ENGINE PAINT

1986 black engine paint is available from WDDGM in 11 oz. aerosol cans, part no. 1052439.

VINYL ROOF MOLDING COLORS

Paint W Inmont Code Code Color Name Ditzler DuPont (R.M.)

11 3967 White 2-130 D8369 4415

19 848 Black 120 D8368 4416

31 8592 Dk. Blue Met. 2-1114 D8556 15060D 43 8572 Lt Sage Met. 2-113 D8557 15182 48 8747 Black Emerald 2-1186 * 16101 63 7260 Lt. Sandstone 2-793 * 12293 74 7384 Aut Maple Met. 2-895 * 12786M 75 8746 Garnet Red Irid 2-1191 * 16101 78 8756 Dk. Carmine Irid 2-1192 * 16103 79 8529 Dk Red Met. 2-1105 D8561 15187F 84 7782 Gunmetal Met. 2-1053 C8481 14040

*Not available at this time.

Paint W Sherwin-Williams Code Code Color Name (Acme/Rogers) Martin-Senour

11 3967 White J4-5676 32-26185 11510 19 848 Black J4-1990 32-16082 9739 31 8592 Dk. Blue Met. 35026 32-26753 43 8572 Lt Sage Met. 35087 32-26761 48 8747 Black Emerald 35771 32-26841 63 7260 Lt. Sandstone 31629 32-26473 74 7384 Aut Maple Met. 32415 32-26560 75 8746 Garnet Red Irid 35770 32-26840 78 8756 Dk. Carmine Irid 35773 32-26843 79 8529 Dk Red Met. 35086 32-26760 84 7782 Gunmetal Met. 34124 32-26705

EXTERIOR PLASTIC PARTS

All 1986 Oldsmobiles have exterior parts made of various types of plastic materials that require specific procedures to obtain high quality refinishing results. Included in this bulletin is a chart listing the different types of plastic materials used on 1986 models. For best results when painting is required, determine the type of plastic material from the chart. Then follow the correct paint procedure, depending upon what painting material and equipment is available.

PLASTIC TYPE SYMBOL

Thermoset Urethane RRIM Thermoplastic Urethane TPU Thermosetting Polyester UP (SMC) Thermoplastic Urethane RIM Thermoplastic Elastomer TPE

1. GENERAL PAINT PROCEDURE FOR EXTERIOR FLEXIBLE PLASTICS

Polyvinylchloride (PVC), Polyurethane (PUR, TPUR, RRIM, RIM), Thermoplastic Elastomer (TPE), Thermoplastic Polyester (SMC), EPDM Rubber (Supplied in Prime).

There are a multitude of finishing systems available on the market for painting and/or repairing flexible plastic parts. Following is a general outline of painting procedures, including a list of available products. Refer to the manufacturer's literature available through your jobber for details on proper mixing and application.

A. Thoroughly clean part by washing with a suitable cleaning solvent* to remove all surface contaminates.

#### NOTICE: Previously painted parts that show signs of cracking, peeling or improper adhesion must be stripped before repainting. The old finish may be removed with any commercially available chlorinated solvent stripper or lacquer thinner.

#### NOTICE: Do not soak parts longer than necessary to remove the old paint to avoid swelling.

B. Scuff sand to an even dull appearance the entire surface to be painted with fine (400 grit or less) sandpaper and feather edge any damaged areas and rewash as in Step A.

#### NOTICE: Unpainted parts do not require sanding prior to painting, but should be thoroughly cleaned as in Step A.

C. Apply two (2) thin coats of primer when required per top coat manufacturer's recommendation and allow to completely dry before proceeding. (For most products, approximately 30 minutes).

D. Prepare color coat according to the manufacturer's recommendation and apply sufficient double coats to develop the proper shade. For best results, allow a few minutes flash time between each double coat and allow to completely dry before using.

E. Following is a list of some of the products available for painting flexible plastic.

Ditzler Elastomeric Primer - DPX844 Ditzler Flexative - DX369 (Permanent Flexible Urethane Additive) Ditzler Flex Additive - DX1798 (Non-Urethane Additive) Ditzler Delthane - DXR80 (Acrylic Enamel Hardner) Rinshed-Mason Acrylic Flex Agent 891 DuPont Dexlar Flexible Finish (Lucite tints plus Dexlar 365B Additive) Sherwin-Williams Flex Additive - V2V297 Acme/Rogers Flex Additive - 699/4699 Martin-Senour Flex Additive - 3082

*Cleaning Solvents 1. DuPont Prep-Sol 2. Rinshed-Mason Pre-Kleano 900 3. DitzLer Acryli-Clean DX330 4. Sherwin-Williams R7K156 5. Acme 88; Rogers 088 6. Martin-Senour 6383

II. NYLON - Will be supplied in prime. Use the same procedure to refinish as on sheet metal parts.

III. ACRYLONNITRILE-BUTADIENE-STYRENE (ABS) - No prime required; paint with acrylic lacquer.

IV. POLYESTER PARTS (UP, PBTP) - Will be supplied in prime and/or black paint. Use the same procedure to refinish or repair as on sheet metal parts.

V. POLYPROPYLENE - Interior parts.

A. Wash surface thoroughly with enamel reducer. (Do not use wax and grease removen.)

B. Apply primer immediately and allow to dry completely before color coating.

C. Color coat with lacquer or enamel reduced and applied according to the manufacturer's recommendation.

D. Materials:

Cleaning Solvent - DuPont 3812S Enamel Reducer Ditzler DTE-101 or DTE-102 "Bobcat" Enamel Reducer Primer - DuPont 3293 GM 1052364

PAINT MATERIAL USAGE BY ASSEMBLY PLANT

Listed below is a current listing of the various GM assembly plants and their suppliers. It should be noted, however, that paint suppliers are subject to change at any given time.

Assembly Plant Paint Type Paint Supplier Paint Codes -------------- ---------- -------------- ----------- Arlington Acrylic Lacquer DuPont All Flint B/C C/C Acrylic Enamels P.P.G. All Detroit B/C C/C Acrylic Enamels DuPont All Doravi Ile Acrylic Lacquer DuPont All Fleetwood Acrylic Lacquer Inmont All Framingham Acrylic Lacquer DuPont All Lansing A-Plant B/C C/C Acrylic Enamels DuPont All B-Plant B/C C/C Acrylic Enamels DuPont All Leeds Acrylic Lacquer DuPont All Orion B/C C/C Acrylic Enamels P.P.G. All Oshawa No . 1 Acrylic Lacquer DuPont All Pontiac Acrylic Lacquer P.P.G. All St. Therese Acrylic Lacquer Inmont All Wentzville B/C C/C Acrylic Enamels Inmont All Willow Run B/C C/C Acrylic Enamels Inmont All

#### Note: B/C C/C = Basecoat Clearcoat

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.