CAMPAIGN:TIRE PLACARD LABEL INFORMATION. Oldsmobile Custom Cruiser 1985

For 1990-2009 cars

# CAMPAIGN:TIRE PLACARD LABEL INFORMATION

#### MODELS/YEARS 1985 DELTA 88 MODELS

#### CONDITION

General Motors has determined that certain 1985 Oldsmobile Delta 88 models fail to conform to Federal Motor Vehicle Safety Standard 110 regarding tire placard requirements. The tire placard label on the left front door of the vehicle may have been printed in error. The error appears on the tire placard label and specifies a higher maximum loading than is allowed. Excessive vehicle loading could cause a tire blowout.

#### VEHICLES INVOLVED

Certain 1985 Delta 88 models assembled at the Detroit plant (9) between and including the following serial numbers:

Plant From Through ----- ---- ------- 9 F9007798 F9010167

#### DEALER ACTION

To reduce the possibility of this occurring on vehicles involved, dealers are to install the labels on all affected vehicles in new and used vehicle stock prior to their sale.

Dealers are to service all vehicles subject to this campaign at no charge to the owner, regardless of mileage, age of vehicle, or ownership, from this time forward.

Whenever a vehicle subject to this campaign is taken into your dealership for service in the future, you should take the steps necessary to be sure the campaign correction has been made before reselling or releasing the vehicle.

Owners of vehicles recently sold from your new vehicle inventory are to be contacted by the dealer, and arrangements made to make the required modification according to instructions contained in this bulletin.

#### SERVICE PROCEDURE

1. Open left front door and clean the surface of the old label with soap and water and wipe dry.

2. Peel new label from paper back and apply both sections of the label over the old label.

3. Install a campaign correction label on the radiator baffle where it is readily visible.

Each vehicle modified in accordance with the instructions outlined in this Product Campaign Builetin will require a "Campaign Identification Label." Each label provides a space to include the five (5) digit dealer code of the dealer performing the campaign service. This information may be inserted with a typewriter or ballpoint pen.

Each "Campaign Identification Label" is to be located on the radiator core support in an area which will be visible when the vehicle is brought in by the owner for periodic servicing.

Apply "Campaign Identification Label" only on a clean dry surface.

#### LABEL INFORMATION

Certification and Tire Placard labels bearing the VIN of each vehicle involved will be forwarded directly to owners of record with instructions for installation. Owners may install the label personally or request that it be installed by your dealership. Should this occur the label is to be installed at no charge to the owner and a claim submitted.

Dealers having vehicles to correct, will be forwarded a specific label for each VIN listed that Oldsmobile records indicate to be in dealer inventory, along with the Campaign Bulletin.

If a label is received mutilated or unusable, please contact your zone office for information on obtaining a duplicate label.

#### WARRANTY INFORMATION

Operation Number Hours --------- ------ ----- Install new label V2640 .2 hr.

.1 hour for clerical administration may be added to the above operation number.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.