For 1990-2009 cars

### Removal Procedure

1. Remove the splash shield from the right front wheelhouse panel. Refer to Wheelhouse Splash Shield Replacement in Body Front End.
2. Remove the splash shield from the left front wheelhouse panel. Refer to Wheelhouse Splash Shield Replacement in Body Front End.
3. Remove the fender to fascia retainers.
4. Remove the retainers (2) from the top of the fascia (4).
5. Remove the retainers (5) from the bottom of the fascia (4).
6. Remove the sidemarker lamps. Refer to Park/Turn Signal/Side Marker Lamp Replacement in Lighting Systems.
7. Remove the fascia (4) from the impact bar (6).

### Installation Procedure

1. Install the fascia (4) to the impact bar (6).
2. Install the sidemarker lamps. Refer to Park/Turn Signal/Side Marker Lamp Replacement in Lighting Systems.
3. Install the retainers (2) to the top of the fascia (4).
4. Install the retainers (5) to the bottom of the fascia (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the fender to fascia retainers.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

6. Install the splash shield to the left front wheelhouse panel. Refer to Wheelhouse Splash Shield Replacement in Body Front End.
7. Install the splash shield to the right front wheelhouse panel. Refer to Wheelhouse Splash Shield Replacement in Body Front End.