For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 3C FRONT SUSPENSION HUB SEAL TOOL

#### SUBJECT: SERVICE MANUAL UPDATE - FRONT SUSPENSION - INNER HUB SEAL INSTALLER ILLUSTRATION LABELED WITH CORRECT TOOL NUMBER

#### MODELS/YEARS: 1991 CUTLASS CALAIS

The 1991 Cutlass Calais Service Manual improperly labels the inner Hub Seal installer. The correct tool number is J 34658.

The illustration below, showing tool #J 34658 replaces the illustration in the current manual. Reference to the tool number must also be corrected on pages 3C-8, 3C-10, and 3C-16 (figure 21).

Please correct your copy(s) of the 1991 Cutlass Calais Service Manual

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.