For 1990-2009 cars

# POWER STEERING PRESSURE HOSE LEAKAGE (REPLACE HOSE)

1987 CUTLASS CIERA MODELS WITH 2.5L ENGINE (RPO LR8)

Some 1987 Cutlass Ciera models with 2.5L engines, (RPO LR8), may exhibit a slight fluid leakage from the power steering pressure hose connector/pipe assembly.

A new power steering pressure inlet hose assembly, part number 26012610, has been released for service usage. This new assembly will replace the existing pressure inlet hose assembly, idle speed switch connector and pressure pipe. (See Figure 1).

Vehicles exhibiting this condition may be repaired by installation of this new hose assembly following applicable shop manual procedure and referring to Figure 2.

#### WARRANTY INFORMATION:

Labor Operation Number: T1322

Labor Time: .5 hrs.

Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.