For 1990-2009 cars

# PASSENGER CAR TOWING INSTRUCTION UPDATE

#### MODELS/YEARS: 1989 CUTLASS CALAIS INTERNATIONAL SERIES

Please update your copy(s) of the 1989 General Motors Towing Instruction Booklet T-60 (red booklet) as follows:

- On Page 48, add the following information under the 'Oldsmobile Calais' heading:

"Except International Series; see Page 52-53"

- On Page 52, add the following information as the third line in the heading:

"Oldsmobile - Cutlass Calais International Series"

Do not tow the Oldsmobile Cutlass Calais International series using sling type equipment. If sling type equipment is used, severe damage to the front or rear fascia will occur.

Wheel lift or car carrier equipment should be used, without exceeding the maximum speed and distance limits for a rear tow (30 mph maximum speed; 50 miles maximum distance). Refer to Illustrations on reverse side of bulletin.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.