For 1990-2009 cars

### Removal Procedure

For the IP cluster indicator lamp bulb locations, refer to Instrument Cluster Replacement .

1. Remove the instrument panel cluster. Refer to Instrument Cluster Replacement .
2. Twist the bulb/socket assembly counterclockwise in order to remove the bulb/socket assembly.

### Installation Procedure

1. Install the bulb into the socket.
2. Install the socket into the cluster.

Turn the socket clockwise in order to tighten the socket.

3. Install the cluster into the instrument panel. Refer to Instrument Cluster Replacement .