For 1990-2009 cars

# REAR SEAT BACK-TO-BACK WINDOW TRIM FINISH PANEL REMOVAL

#### MODELS/YEARS: 1987 "A-37" STYLE (BODY TYPE VIN CODE 1)

The service procedure for the Cutlass Ciera, "A-38" style, rear seat back-to-back window trim finishing panel assembly was omitted from the Seat Section (9A) of the 1987 Body Service Manual.

The following service procedure has been provided and should be used as reference when a trim panel is removed or installed.

#### SERVICE PROCEDURE

#### Remove or Disconnect (Figure 1)

1. Retaining tabs on underside of stowage compartment (not shown)

2. Center high mounted stop lamp cover and lamp assembly (3). See Section 7 of the Body Service Manual.

3. Rear seet cushion and back

4. Left and right quarter trim panels

5. Speaker grilles, if present

6. Screws (2), if present

7. Retainer (4), if present

8. Trim panal to seat back adhesive bond (5)

9. Rear seat back to back window trim panel (1)

#### Install or Connect

1. Rear seat back to back window trim panel (1)

2. Trim panel to seat back (5). Use nonstaining adhesive.

3. Retainer (4)

4. Screws (2)

5. Speaker grilles

6. Quarter trim panels

7. Rear seat cushion and back

8. Lamp assembly and cover

9. Retaining tabs

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.