For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector at the EGR valve.
2. Remove the two base to flange nuts and linear EGR valve assembly.

### Installation Procedure

1. Install the linear EGR valve assembly - two nuts.

Tighten
Tighten the nuts to 30N·m (22 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Connect the electrical connector.