For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 39232 Wiper Transmission Separator

1. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .
2. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement in Body Front End.
3. Disconnect the electrical connector from the wiper motor.
4. Remove 3 screws and the wiper drive system module from the vehicle.
5. Remove the 3 grommets and the 2 caps from the wiper transmission.
6. Remove the drive link from the wiper motor crank arm using the J 39232 .
7. Remove 2 screws and the wiper motor from the tube frame.

### Installation Procedure

#### Tools Required

J 39529 Wiper Transmission Installer

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the wiper motor onto the tube frame with the 2 screws.

Tighten
Tighten the 2 screws to 10 N·m (88 lb in).

2. Install the drive link onto the wiper motor crank arm using the J 39529 .
3. Install the 3 grommets and the 2 caps on the wiper transmission.
4. Install the wiper drive system module onto the vehicle with the 3 screws.

Tighten
Tighten the 3 screws to 10 N·m (88 lb in).

5. Connect the electrical connector onto the wiper motor.
6. Install the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement in Body Front End.
7. Install the wiper arms. Refer to Windshield Wiper Arm Replacement .
8. Operate the wipers and inspect for proper operation.