For 1990-2009 cars

# FUEL PUMP NOISE ON COUPES & SEDANS WITH V-6 ENGINE

#### MODELS/YEARS: 1984-87 CUTLASS CIERA SEDANS AND COUPES WITH V-6 ENGINES (VIN CODE W OR 3)

Some 1984-87 Cutlass Ciera sedans and coupes with V-6 engines (Vin Codes W or 3) may exhibit what is considered to be an objectionable level of fuel pump noise audibile in the vehicle passenger compartment.

The objectionable level of noise may be attributed to any of the components or conditions noted below:

1. Fuel pump 2. Pulsator 3. Inadequate pump discharge port to sender feed pipe clearance 4. Improper tank to underbody position/isolation resulting in ground out

Vehicles exhibiting this condition may be repaired by following the procedure below:

1. Drain and lower fuel tank following applicable service manual procedures in Section 6C.

2. Remove existing anti-squeak material from tank and discard.

3. Clean top of fuel tank and remove fuel sender/pump assembly.

4. Remove and discard pulsator. Inspect to insure a minimum distance of 1/4 inch exists between pump discharge port and sender feed pipe, (Figure 1). Replace sender as required (see GMSPO parts catalog for correct application).

5. Inspect pump under foam isolation sleeve for part number. If part number is either 6442409 or 6442439 replace pump (see GMSPO part catalog for correct application).

6. Reassemble sender/pump assembly utilizing new pulsator, part number 25093965, insuring pump and pulsator are positioned properly (Figure 1).

7. Install pump and sender in tank without sealing "O" ring. If sender cover does not rest on the "O" ring seat, the pump is bottoming out on the tank bottom in which case it will be necessary to obtain clearance.

8. Remove sender assembly and reinstall using a new sender sealing "O" ring, part number 22515965.

9. Cut each of the long isolation strips contained in sound isolation kit, part number 22530899, to lengths noted below: 2 pieces - 3 1/2" 2 pieces - 4 1/2" 1 pieces - 8"

10. Position isolation material to top of fuel tank, (Figure 2).

11. Position and secure fuel line separator contained in isolation kit as shown by applicable model year (Figure 3).

12. Raise and position fuel tank to vehicle underbody. Loosely attach straps to underbody placing two 7/16" flat washers, part number 3899696, or equivalent on each of the strap bolts between strap and underbody attaching point (Figure 4).

13. Insure fuel tank strap spacer located on L.H. strap is properly positioned under forward flange to tank (Figure 5). Torque L.H. strap bolt and then R.H. bolt to 34 N.m (25 lbs. ft.).

14. Inspect to insure forward tank flange is not contacting strap body bracket, and that sender pipes are not in contact with either tank or underbody. Correct as required.

15. Reconnect fuel hoses and electrical connector following service manual procedure, Section 6C.

16. Start car, inspect for any fuel leakage and repair as necessary.

Parts that are required for this procedure, are available from GMSPO and are noted below excluding applicable pump and sender part numbers which can be obtained from GMSPO parts catalog.

Part Number Description Quantity Required ----------- ----------- ----------------- 22530899 Sound Isolation Kit 1 25093965 Pulsator 1 3899696 7/16" Flat Washer or Equivalent 4 *22515965 Fuel Sender "O" ring 1

*"O" ring is included with fuel sender or pump service kit and separate ordering is not required when either of these components are replaced.

Labor Operation Number: T5122 Labor Time: 1.1 hrs.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.