For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement .
2. Squeeze the oblong connector at the following locations in order to disconnect the cables:

• | The motors

• | The vertical/horizontal actuators

### Installation Procedure

1. Connect the cables by pushing to the connector until you hear an audible click is heard.
2. Install the front seat. Refer to Seat Replacement .