For 1990-2009 cars

1. Remove the ten channel plate bolts (8 and 25).
2. Remove the channel plate assembly (27). Keep the following components with the channel plate:

• | The drive sprocket to channel plate thrust washer (34)

• | The three accumulator pistons (29)

• | The manual valve (800)

• | The detent lever spring (804) and bolt (805)

3. Remove and discard the channel plate to case gasket (28).