For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment lid lock cable assembly latch.
2. Remove the rear compartment lid applique. Refer to Rear Compartment Lid Applique Replacement .
3. Remove the rivets (2).
4. For Oldsmobile models, remove the rear compartment lid lock cylinder (3) and shim.
5. For Chevrolet models, remove the rear compartment lid lock cylinder gasket (1).

### Installation Procedure

1. For Chevrolet models, install the rear compartment lid lock cylinder gasket (1).
2. For Oldsmobile models, install the rear compartment lid lock cylinder (3) and shim.
3. Install the rivets (2).
4. Install the rear compartment lid applique. Refer to Rear Compartment Lid Applique Replacement .
5. Install the rear compartment lid lock cable assembly latch. Ensure that the latch is fully seated. This action will engage the locking tabs.