For 1990-2009 cars

# 6000 MANUAL UPDATE PAGE OMITTED FROM MANUAL

#### VEHICLES AFFECTED: 1985 6000 --------- 'The attached page was omitted from the 1985 6000 Service Manual. Please include these pages with your copy of the manual'.

TRIM HEIGHTS (@ CURB WEIGHT) ---------------

"Z, D,J and K" DIMNESIONS- LIFT BUMPER OF VEHICLE UP APPROXIMATELY 38mm. GENTLY REMOVE HANDS AND LET VEHICLE SETTLE REPEAT TWICE FOR A TOTAL OF 3 TIMES. MEASURE "Z" AND "J" DIMENSIONS. PUSH BUMPER DOWN APPROXIMATELY 38mm. GENTLY REMOVE HANDS AND LET VEHICLE RISE ON ITS OWN. REPEAT TWICE FOR A TOTAL OF 3 TIMES. MEASURE DIMENSIONS. TRUE HEIGHTS ARE THE AVERAGE OF THE HIGH AND LOW MEASUREMENTS.

#### RECOMMENDED TIRE PRESSURE

TRIM HEIGHT - SET PRESSURE TO AGREE WITH VEHICLE TIRE PRESSURE STICKER FOR LOADING "UP TO VEHICLE CAPACITY."

#### LOAD CONDITIONS

CURB WEIGHT - VEHICLE IS BUILT TO PARTS LIST SPECIFICATIONS INCLUDING COOLANT TO CAPACITY AND FULL TANK OF GASOLINE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.