For 1990-2009 cars

### Removal Procedure

1. Remove the rear panel trim. Refer to Rear Window Trim Panel Replacement .
2. Lift the retainers. Slide the tabs from the slots.
3. Remove the high mount stoplamp (1).

### Installation Procedure

1. Push the high mount stoplamp tabs downward into the slots until the tabs are secure.
2. Install the rear panel trim. Refer to Rear Window Trim Panel Replacement .