For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 37043 Parking Brake Release

• | J 38400 Brake Shoe Spanner and Spring Removal

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Disconnect the right rear park brake cable (2) from the cable connector (1).
3. Disconnect the right rear park brake cable (1) from the bracket (3) using the J 37043 .
4. Remove the tire and wheel assembly. Refer to Wheel Removal .
5. Remove the brake drum.
6. Remove the brake shoes (1). Refer to Brake Shoe Replacement .
7. Disconnect the cable from the parking brake lever (7).
8. Remove the cable from the backing plate (5) using the J 37043 .

### Installation Procedure

Notice: Parking brake adjustment is not necessary. This is a self adjusting system and damage may result from attempting to adjust or modify this system in any way. It may be necessary to adjust the rear brakes to obtain the proper tension in the system.

1. Install the cable to the backing plate (5).
2. Connect the cable to the parking brake lever (7).
3. Install the brake shoes. Refer to Brake Shoe Replacement .
4. Install the brake drum.
5. Install the tire and wheel assembly. Refer to Wheel Installation .
6. Connect the right rear park brake cable (1) to the bracket (3).
7. Connect the right rear park brake cable (2) to the cable connector (1).
8. Lower the vehicle.