For 1990-2009 cars

# 1980 REAR BRAKE ASSEMBLY FOUND ON 1981 MODELS

SOME 1981 CUTLASS MODELS WILL HAVE 1980 MODEL REAR BRAKE ASSEMBLIES. THE DIFFERENCE BETWEEN THE TWO BRAKE ASSEMBLIES IS IN THE CONFIGURATION OF WHEEL CYLINDER PILOT AND THE CORRESPONDING HOLE IN THE BACKING PLATE AS SHOWN IN FIG. 2. WHEN MAKING REPAIRS ON A 1981 CUTLASS CHECK TO DETERMINE IF THERE IS A 1980 BACKING PLATE AND WHEEL CYLINDER. IF EQUIPPED WITH 1980 PARTS BE SURE TO ORDER THE CORRECT PART NUMBER.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.