For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6A ENGINE MECHANICAL-OIL PAN

#### SUBJECT: SERVICE MANUAL UPDATE OIL PAN AND GASKET REPLACEMENT PROCEDURE

#### MODELS/YEARS: 1989-91 CUTLASS CIERA W/2.5L (VIN R)

The following Oil Pan and Gasket Replacement procedure updates and replaces the procedure found in the 1989-91 Cutlass Ciera and Cruiser Service Manuals - Section 6A, on pages 6A1-13 (1989), 6A1-20 (1990), and 6A1 -27 (1991). This change is due to a new labor time study.

Remove or disconnect

1. Negative battery cable. 2. Air cleaner and duct assembly. 3. Serpentine belt. 4. Engine torque strut from engine bracket. 5. Two upper front A/C compressor bolts to mounting bracket. 6. Install J 28467-A. 7. Raise vehicle and suitably support. (Refer to General Information 0A). 8. Right front tire and wheel assembly. (Refer to Tires and Wheels 3E). 9. Right engine splash shield. 10. Exhaust pipe and converter. 11. Lower front A/C compressor mounting bolts and support brace. 12. Rear A/C compressor mounting bracket bolts. 13. Wire harness from bracket at transaxle. 14. Flywheel cover bolts. 15. Starter and support bracket, set aside. 16. Flywheel cover. 17. Engine support bracket bolts to engine. 18. Loosen transaxle mounting nuts. 19. Lower vehicle. 20. Raise front of engine about 3 inches using J 28467-A. 21. Engine support bracket nuts to engine mount and frame assembly. Remove support bracket and mount. (Refer to Frame and Underbody-Sec. 10-3). 22. Raise vehicle and suitably support. (Refer to General Information-Sec. 0A). 23. Drain engine oil. 24. Using a jack stand, place a wood support along transaxle oil pan inside edge. Raise transaxle and engine assembly to normal sitting position using J 28467-A. 25. Oil pan retaining bolts. 26. Oil pan from engine block.

Clean engine block and oil pan surfaces.

#### Install or connect

1. Apply RTV sealer GM P/N 12345739 or equivalent. 2. Oil pan to engine block. 3. Tighten oil pan retaining bolts to 10 N-m (89 lbs. in.). 4. Remove lack stand and wood support. 5. Lower vehicle. 6. Fill engine oil. (Refer to Maintenance and Lubrication 0B). 7. Nuts holding engine support,bracket to engine mount and mount assembly to frame assembly, bracket and mount. 8. Lower front of engine. 9. Raise vehicle. 10. Tighten transaxle mounting nuts 50 N - m (37 lbs. ft.). 11. Engine support bracket bolts to engine and tighten to 50 N-m (37 lbs. ft.). 12. Flywheel cover. 13. Starter assembly and support bracket. (Refer to Cranking System 6D2). 14. Tighten flywheel cover bolts to 1 0 N - m (89 lbs. in.). 15. Wire harness to bracket at transaxle. 16. Tighten rear A/C compressor mounting bracket bolts to 30 N - m (22 lbs. ft.). 17. Lower front A/C compressor mounting bolts and support brace and tighten to 25 N - m (18 lbs. ft.). 18. Exhaust pipe and converter. 19. Right engine splash shield. 20. Right front tire and wheel assembly. (Refer to Tires and Wheels-3E). 21. Lower vehicle. 22. Remove J 24867-A. 23. Tighten upper front A/C compressor to mounting bracket bolts to 25 N-m (18 lbs. ft.). 24. Engine torque strut to engine bracket and tighten to 56 N-m (41 lbs. ft.). 25. Serpentine belt. 26. Air cleaner and duct assembly. 27. Negative battery cable.

Inspect for oil level and leaks.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.