For 1990-2009 cars

# CAMPAIGN: INCORRECT TRANSAXLE DIPSTICK READING-440T4

#### MODELS/YEARS ALL 1984 & EARLY PRODUCTION 1985 CUTLASS CIERAS EQUIPPED WITH A 3.8L MPFI ENGINE & 440-T4 TRANSAXLE

CONDITION

General Motors has determined that all 1984 and some early production 1985 Cutiass Cieras equipped with a 3.8L MPFI engine and 440-T4 transaxle were assembled with transaxle oil filler tube and dipstick combinations which give an incorrect oil level reading. The transaxles on these vehicles were properly filled at time of manufacture as the dipsticks are not used by the assembly plants to determine the oil level.

If a dealer or service facility should accurately check and adjust the transaxle fluid level according to the dipstick reading on one of these vehicles, the transaxle would be approximately two (2) pints low of fluid. This low fluid level could result in transaxle slippage in cold weather and during certain maneuvers, resulting in damage to the transaxle.

#### VEHICLES INVOLVED

All 1984 Cutlass Cieras equipped with a 3.8L MPFI engine and 440-T4 transaxle.

1985 Cutlass Cieras equipped with a 3.8L MPFI engine and 440-T4 transaxle within the following serial numbers:

Beginning Up To Assembly Plant Start of Production and Including -------------- ------------------- ------------- Doraville (D) SOP FD407657 Framingham (G) SOP FG365201 Oshawa (9) SOP F9300025

Some 1985 Cutlass Cieras with a 3.8L MPFl engine and 440-T4 transaxle which have VINs higher than those listed, were assembled with an interim dipstick, part number 25519030B, these dipsticks are the same length and design as the new part. Do not replace these dipsticks. Refer to Figure 1.

#### DEALER ACTION

To prevent the possibility of this condition occurring on vehicles involved, the original transaxle dipstick is to be replaced with a new correct reading dipstick, part number 25527122. Refer to Figure 1 to identify the old and the new dipstick.

Since dipsticks can be installed very easily, and because we do not want to cause owners unnecessary inconvenience, the new dipsticks have been furnished directly to affected owners of record. Owners may install them personally or they may request dealer assistance for installation.

Dealers are to perform this recall campaign at no charge to the owner, on affected vehicles, regardless of time, mileage or ownership, and are to correct all affected vehicles in dealer new and used car inventory prior to their sale.

Whenever a vehicle subject to this campaign is taken into your new or used car inventory in the future, you should take the steps necessay to be sure the campaign correction has been made before reselling the vehicle.

#### SERVICE PROCEDURE

1. Raise the hood of the vehicle, locate the transaxle dipstick and replace it with the dipstick furnished.

2. After the above has been completed, install a campaign correction label as follows: record campaign number 85-C-05, dealer code and date on the blank campaign correction label and install on the radiator support where it is readily visible.

#### PARTS INFORMATION

The correct quantity of transaxle dipsticks are being shipped to each dealer on a "NO CHARGE" basis (only for VINs on your list with no owner name). They WILL NOT BE billed on dealer parts account. Dealers should not order from WDDGM. If transfers make additional parts necessary, contact your zone office.

Replaced parts are to be retained for disposition by zone personnel.

WARRANTY CLAIM INFORMATION

Description Failure Code Labor Operation Labor Hours ----------- ------------ --------------- ----------- Install New 96 V2900 .2 Dipstick

A parts credit for 30% of dealer price of the "furnished" transaxle dipstick will be credited to the above operation number.

.1 hour for clerical administration may be added to the above operation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.