For 1990-2009 cars

# SERVICE MANUAL UPDATE STARTER MOTOR REPLACEMENT

#### MODELS/YEARS: 1988 CUTLASS CIERA, PAGES 6D-2-3-4

The cranking motor procedure in the 1988 Service Manual has been revised. The following procedure should be used when removing or installing the cranking motor:

#### CRANKING MOTOR

#### REMOVE OR DISCONNECT

1. Negative batery cable.

2. Engine side strut bolt and upper radiator panel bracket.

3. Engine side strut bracket.

4. Discharge A/C system refer to Air Conditioning (Section 1 B).

5. Raise vehicle, refer to General Information (Section OA).

6. Cooling fan lower retaining bolts and disconnect electrical connection at fan.

7. Lower vehicle.

8. Cooling fan upper.

9. 3 spark plug wires and oil indicator tube assembly.

10. Exhaust manifold flange bolts.

11. Exhaust manifold bolts and manifold.

12. A/C manifold retaining bolt from A/C compressor and remove A/C line retaining bolt.

13. Starter wiring from starter.

14. Ralse vehicle, refer to General Information (Section OA).

15. Flywheel inspection cover.

16. Starter mounting bolts and starter (shims, if used).

#### INSTALL OR CONNECT

1. Shims, starter and mounting bolts Tighten bolts to 40 N.m (30 lb. ft.)

2. Flywheel inspection cover.

3. Wiring to starter.

4. A/C manifold bolt and A/C line bracket bolt.

5. Lower vehicle.

6. Exhaust manifold.

7. Exhaust manifold flange bolts.

8. Oil indicator tube assembly and connect spark plug wires.

9. Cooling fan assembly, install upper retaining bolts.

10. Raise vehicle, refer to General I nformation (Section OA) .

11. Connect electrical connections to fan, cooling fan lower retaining bolts.

12. Lower vehicle.

13. Engine side strut bracket.

14. Upper radiator panel bracket, strut and bracket bolts.

15. Connect negative battery cable.

16. Evacuate and charge A/C, refer to Air Conditioning (Section 1 B).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.