For 1990-2009 cars

#### Automatic Transaxle C102

Connector Part Information |

• | 12160493

• | 20-Way F Micro-Pack 100 Series (GRY)

Connector Part Information

• | 12160782

• | 20-Way M Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | LT GRN | 1222 | Shift Solenoid A Output | A | LT GRN | 1222 | Shift Solenoid A Output
B | YEL/BLK | 1223 | Shift Solenoid B Output | B | YEL | 1223 | Shift Solenoid B Output
C | RED/BLK | 1228 | Transaxle Force Motor Feed | C | PPL | 1228 | Transaxle Force Motor Feed
D | LT BLU/WHT | 1229 | Transaxle Force Motor Return | D | LT BLU | 1229 | Transaxle Force Motor Return
E | PNK | 1039 | Fuse Output, Ignition 1 | E | RED | 839 | Fuse Output, Ignition 1
F-K | -- | -- | -- | F-K | -- | -- | --
L | YEL/BLK | 1227 | Transaxle Temperature Sensor Signal | L | BRN | 1227 | Transaxle Temperature Sensor Signal
M | BLK | 452 | Sensor Return | M | GRY | 452 | Sensor Return
N | PNK | 1224 | Transaxle Pressure Switch Signal (Bit 1) | N | PNK | 1224 | Transaxle Pressure Switch Signal (Bit 1)
P | RED | 1226 | Transaxle Pressure Switch Signal (Bit 3) | P | ORN | 1226 | Transaxle Pressure Switch Signal (Bit 3)
R | DK BLU | 1225 | Transaxle Pressure Switch Signal (Bit 2) | R | DK BLU | 1225 | Transaxle Pressure Switch Signal (Bit 2)
S | RED/BLK | 1230 | Transaxle Input Speed Sensor Signal | S | BLK | 1230 | Transaxle Input Speed Sensor Signal
T | BRN | 418 | TCC Solenoid Output (Pulse Width) | T | TAN | 418 | TCC Solenoid Output (Pulse Width)
U | YEL | 657 | TCC Oil Pressure Switch Signal | U | WHT | 1804 | TCC Oil Pressure Switch Signal
V | DK BLU/WHT | 1231 | Transaxle Input Speed Sensor Return | V | DK GRN | 1231 | Transaxle Input Speed Sensor Return
W | -- | -- | -- | W | -- | -- | --