For 1990-2009 cars

# TIE ROD ADJUST CLAMP BOLT NEW TORQUE SPECIFICATION

VEHICLE AFFECTED: 1985 'J' & 'N' Series Vehicles ------------------------------

The torque specification for 1985 'J' and 'N' series vehicle tie rod adjuster clamp bolts has been changed from the 1984 'J' series Service Manual Specification.

Anytime that a toe-in adjustment or other service is performed which requiring retightening of the tie rod adjust clamp bolts, the bolts must be retigthened to 55N.m (41 lbs. ft.).

When inner or outer tie rod service parts are replaced on past model 'J' series vehicles, the adjuster clamp bolts must also be retightened to 55N.m (41 1bs. ft.).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.