For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 10 UNDER BODY DIMENSION CHANGE

#### Subject: SERVICE MANUAL UPDATE - SECTION 10 (UNDERBODY, ENGINE COMPARTMENT, FRONT DOOR AND HOOD HINGE DIMENSIONS CHANGE)

#### Models Affected: 1982 - 1991 CUTLASS CIERA/CUTLASS CRUISER

Due to a redesigned front fender wheelhouse panel, the body alignment dimensions and measurement locations at the strut towers have changed. Reference Point "D" has changed from the center of strut shock tower front attaching hole, to the center of the strut shock tower 90mm (3-9/16") hole.

The following information replaces Figures 2, 3, 4, 7 and 8 in the 1991 Pontiac 6000 Service Manual, Section 10-3.

Section 10-3 with these revised dimensions should be used for all prior model year Cutlass Cieras and Cutlass Cruisers replacing any information in prior manuals referring to the frame and underbody.

REF. HORIZONTAL VERTICAL LOCATION --- ---------------- ---------------- ----------------- A Leading edge Upper surface at Motor compartment corner front panel,

B Center of 16mm (5/8") Lower surface at gage Front end lower tie gage hole bar, outboard of frame attaching hole

C Center of 18 mm None Motor compartment (11/16") gage hole side rail

D Center of strut Upper surface at Strut shock tower shock tower 90mm strut shock tower (3-9/16") hole

E Center of front Upper surface at hinge Front upper door upper hinge pin pin hole hinge, body side hole

F Center of 9mm None Engine compartment (23/64") gage hole side rail

G Center of outboard None Hood hinge end of hood hinge pivot pin

H Center of 16mm Lower surface at Reinforcement #1 floor (5/8") gage hole gage hole pan bar, inboard of frame attachment hole

I Center of 16mm Lower surface at Engine compartment (5/8") gage hole gage hole side rail, rearward and outboard of slot in rail

J Center of 20mm Lower surface at Compartment pan (13/16") gage hole gage hole longitudinal rail, forward of control arm reinforcement

K Center of control Lower surface at Compartment pan arm rear inboard rear inboard longitudinal rail attaching hole attaching hole control arm reinforcement

L Front edge of Lower surface at Compartment pan 20mm (13/16") gage hole longitudinal rail, gage hole rearward of slot in rail

M Center of front Lower surface at Engine frame frame attaching front attaching hole hole

N Center of rear frame None Engine frame attaching hole

0 None Lower surface of Engine frame frame at cross member

P None Upper surface of Engine frame frame at rear edge

Q Center of front None Motor compartment end sheet metal front panel diagonal brace outboard attaching hole

R Center of front None Motor compartment end sheet metal side and diagonal brace wheel house panel attaching hole

Figure 7 Measurement Locations

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.