For 1990-2009 cars

# SERVICE MAN.UPDATE SEC.3E WHEEL NUT TORQUE

SERVICE MANUAL UPDATE

#### SECTION 3E

WHEN INSTALLING WHEEL NUTS, USE THE FOLLOWING TORQUE SPECIFICATION AND TIGHTEN IN THE PROPER SEQUENCE SHOWN ON PAGE 3E-5 OF THE FOLLOWING 1991 SERVICE MANUALS.

1991 PONTIAC 6000 PAGES 3E-5, 10

1991 BUICK CENTURY PAGES 3E-5, 10

1991 OLDSMOBILE CUTLASS CIERA AND CUTLASS CRUISER PAGES 3E-5, 10

WHEEL NUT TORQUE FOR ABOVE MODELS..............140 N.M (100 LBS. FT.)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1990 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED. <