For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC.0B1B A/C CHARGING CAPACITY SPEC.

SERVICE MANUAL UPDATE

#### SECTION 0B

THE R-12 CHARGING CAPACITY SPECIFICATION FOUND IN SECTION 0B MAINTENANCE AND LUBRICATION AND SECTION 1B AIR CONDITIONING HAS BEEN REVISED. THE REVISED SPECIFICATION FOR R-12 CHARGING IS 1.08 KG (2.375 LBS.) FOR ALL 1989-91 "A" CARS, EXCEPT THE PONTIAC 6000 STE MODEL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1991 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.