For 1990-2009 cars

### Removal Procedure

1. Remove the rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.
2. Disconnect the radio rear speaker retainers (1).
3. Remove the radio rear speaker (3).
4. Disconnect the electrical connector (2) from the speakers (3).

### Installation Procedure

1. Connect the electrical connector (2) to the radio rear speaker (3).
2. Install the radio rear speaker (3).
3. Engage the radio rear speaker retainers.
4. Install the rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.