For 1990-2009 cars

### Removal Procedure

1. Lower the window to the full down position.
2. Remove the door outer belt sealing strip. Refer to Outer Belt Sealing Strip Replacement .
3. Remove the door window frame applique. Refer to Door Frame Applique Replacement .
4. Disengage the door upper auxiliary sealing strip fasteners (1).
5. Disengage the door upper auxiliary sealing strip from the door frame (1).

### Installation Procedure

1. Engage the door upper auxiliary sealing strip to the door frame (1).
2. Engage the door upper auxiliary sealing strip fasteners.
3. Install the door window frame applique. Refer to Door Frame Applique Replacement .
4. Install the door outer belt sealing strip. Refer to Outer Belt Sealing Strip Replacement .