For 1990-2009 cars

Table 1: | Auxiliary Power Outlet
Table 2: | Cigar Lighter
Table 3: | Ignition Switch C1
Table 4: | Ignition Switch C2
Table 5: | LH IP Junction Block C1
Table 6: | LH IP Junction Block C2
Table 7: | LH IP Junction Block C3
Table 8: | RH IP Junction Block C1
Table 9: | RH IP Junction Block C2
Table 10: | RH IP Junction Block C3
Table 11: | Underhood Junction Block C1 (LD9 Only)
Table 12: | Underhood Junction Block C1 (L82 Only)
Table 13: | Underhood Junction Block C2
Table 14: | Underhood Junction Block C3
Table 15: | Underhood Junction Block C4
Table 16: | Underhood Junction Block C5
Table 17: | Underhood Junction Block C6
Table 18: | Underhood Junction Block C7

#### Auxiliary Power Outlet

Connector Part Information |

• | 12176836

• | 3-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 40 | Fuse Output, Battery
B | -- | -- | Not Used
C | BLK | 250 | Ground

#### Cigar Lighter

Connector Part Information |

• | 12176836

• | 3-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 40 | Fuse Output, Battery
B | -- | -- | Not Used
C | BLK | 250 | Ground

#### Ignition Switch C1

Connector Part Information |

• | 12110075

• | 6-Way F Metri-Pack Mixed Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 242 | Fuse Output, Battery
B | YEL | 5 | Ignition Switch Output (CRANK)
C | ORN | 300 | Ignition Switch Output (Ignition 3)
D | LT GRN | 80 | Key Reminder Switch Signal
E | DK GRN | 500 | Ignition Switch Output (Ignition 0)
F | -- | -- | Not Used

#### Ignition Switch C2

Connector Part Information |

• | 12162229

• | 6-Way F Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 842 | Fuse Output, Battery
B | PNK | 3 | Ignition Switch Output (Ignition 1)
C | BRN | 4 | Ignition Switch Output (ACCY)
D | -- | -- | Not Used
E | BLK/WHT | 151 | Power Mirror Motor Ground (Clean)
F | -- | -- | Not Used

#### LH IP Junction Block C1

Connector Part Information |

• | 12177208

• | 68-Way F Metri-Pack 280 Series (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | -- | -- | Not Used
A2 | BRN | 4 | Ignition Switch (ACCY)
A3 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
A4 | PNK | 3 | Ignition Switch Output (Ignition 1)
A5-A6 | -- | -- | Not Used
A7 | DK GRN | 500 | Ignition Switch Output (Ignition 0)
A8-A11 | -- | -- | Not Used
A12 | ORN | 1440 | Fuse Output, Battery
B1 | YEL | 43 | Fuse Output, ACCY
B2 | YEL | 143 | Fuse Output, ACCY
B3 | -- | -- | Not Used
B4 | PNK | 739 | Fuse Output, Ignition 1
B5 | -- | -- | Not Used
B6 | YEL | 1139 | Fuse Output, Ignition 1, SIR
B7 | PPL | 1500 | Fuse Output, Ignition 0
B8-B10 | -- | -- | Not Used
B11 | ORN | 1440 | Fuse Output, Battery
B12 | -- | -- | Not Used
C1 | -- | -- | Not Used
C2 | YEL | 143 | Fuse Output, ACCY
C3 | ORN | 1040 | Fuse Output, Battery
C4 | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile)
C5 | RED | 442 | Fuse Output, Battery
C8 | -- | -- | Not Used
C9 | PPL | 1600 | Fuse Output, Ignition 0
C10-C11 | -- | -- | Not Used
C12 | ORN | 1140 | Fuse Output, Battery
D1 | -- | -- | Not Used
D2 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
D3 | -- | -- | Not Used
D4 | BLK | 1576 | Trunk Release Switch Output
D5-D12 | -- | -- | Not Used
E1-E2 | -- | -- | Not Used
E3 | PPL | 1807 | Serial Data Signal, Class B, 10400 Baud (Primary)
E4 | WHT | 156 | Courtesy Lamp Output
E5 | -- | -- | Not Used
E6 | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile)
E7 | ORN | 1540 | Fuse Output, Battery
E8 | -- | -- | Not Used
E9 | ORN | 1732 | Inadvertent Power Control (12 V)
E10 | BLK | 150 | Ground
E11 | -- | -- | Not Used
E12 | RED | 642 | Fuse Output, Battery
F1-F2 | -- | -- | Not Used
F3 | YEL | 1737 | Transaxle Mounted Neutral Safety Switch Output
F4-F5 | -- | -- | Not Used
F6 | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile)
F7-F12 | -- | -- | Not Used

#### LH IP Junction Block C2

Connector Part Information |

• | 12176739

• | 30-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BLK | 470 | Sensor Return
A2-A11 | -- | -- | Not Used
A12 | LT BLU | 1134 | Park Brake Switch Signal
B1 | GRY | 120 | Fuel Pump Motor Feed
B2 | PPL | 30 | Fuel Gauge Sensor Signal
B3 | -- | -- | Not Used
B4 | LT GRN/BLK | 394 | Door Handle Switch Signal, Left Front
B5 | TAN | 201 | Speaker Feed, Left Front
B8-B11 | -- | -- | Not Used
B12 | PPL | 420 | Brake Pedal Switch Output (TCC)
C1 | PPL | 293 | Rear Defogger Element Feed
C2 | BRN | 241 | Fuse Output, Ignition 3
C3 | WHT | 156 | Courtesy Lamp Output
C4 | DK GRN/WHT | 1135 | Brake Transaxle Shift Interlock Solenoid Feed
C5 | GRY | 118 | Speaker Return, Left Front
C8 | -- | -- | Not Used
C9 | ORN | 1732 | Inadvertent Power Control (12 V)
C10-C11 | -- | -- | Not Used
C12 | LT BLU | 1134 | Park Brake Switch Signal

#### LH IP Junction Block C3

Connector Part Information |

• | 12176740

• | 30-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 140 | Fuse Output, Battery
A2 | GRY | 295 | Power Door Lock Motor Feed (LOCK)
A3 | LT BLU | 195 | Power Door Lock Motor Feed (UNLOCK)
A4 | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
A5 | WHT | 194 | Power Door Lock Relay Feed (UNLOCK)
A8 | ORN | 540 | Fuse Output, Battery
A9 (-AUO) | BLK/WHT | 56 | Trunk Release Motor Feed
A9 | GRY | 382 | Trunk Release Enable Relay Output (Common Contact)
A10 | YEL | 1737 | Transaxle Mounted Neutral Safety Switch Output
A11 | ORN | 1040 | Fuse Output, Battery
A12 | BLK | 470 | Sensor Return
B1 | PPL | 420 | Brake Pedal Switch Output (TCC)
B2 | GRY | 295 | Power Door Lock Motor Feed (LOCK)
B3 | LT BLU | 195 | Power Door Lock Relay Feed (LOCK)
B4 | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
B5 | WHT | 194 | Power Door Lock Relay Feed (UNLOCK)
B8 | TAN | 201 | Speaker Feed, Left Front
B9 | LT GRN/BLK | 394 | Door Handle Switch Signal, Left Front
B10 | ORN | 1840 | Fuse Output, Battery
B11 | PPL | 30 | Fuel Gauge Sensor Signal
B12 | GRY | 120 | Fuel Pump Motor Feed
C1 | LT BLU | 1134 | Park Brake Switch Signal
C2 | -- | -- | Not Used
C3 | ORN | 1732 | Inadvertent Power Control (12 V)
C4 | ORN | 1732 | Inadvertent Power Control (12 V)
C5 | ORN | 1240 | Fuse Output, Battery
C8 | GRY | 118 | Speaker Return, Left Front
C9 | DK GRN/WHT | 1135 | Brake Transaxle Shift Interlock Solenoid Feed
C10 | WHT | 156 | Courtesy Lamp Output
C11 | BRN | 241 | Fuse Output, Ignition 3
C12 | BLK | 293 | Rear Defogger Element Feed

#### RH IP Junction Block C1

Connector Part Information |

• | 12177208

• | 68-Way F Metri-Pack 280 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 1740 | Fuse Output, Battery
A2 | ORN | 340 | Fuse Output, Battery
A3-A4 | -- | -- | Not Used
A5 | BRN | 641 | Fuse Output, Ignition 3
A6-A12 | -- | -- | Not Used
B1 | -- | -- | Not Used
B2 | RED | 1042 | Fuse Output, Battery
B3 | -- | -- | Not Used
B4 | BRN | 341 | Fuse Output, Ignition 3
B5 | -- | -- | Not Used
B6 | BRN | 441 | Fuse Output, Ignition 3
B7-B12 | -- | -- | Not Used
C1-C3 | -- | -- | Not Used
C4 | BRN | 341 | Fuse Output, Ignition 3
C5 | ORN | 300 | Ignition Switch Output (Ignition 3)
C8-C12 | -- | -- | Not Used
D1-D12 | -- | -- | Not Used
E1 | -- | -- | Not Used
E2 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
E3 | PPL | 34 | Fog Lamp Feed
E4 | PPL | 34 | Fog Lamp Feed
E5-E10 | -- | -- | Not Used
E11 | GRY | 8 | IP Lamp Feed
E12 | BRN/WHT | 230 | IP Lamps Dimmer Module Output
F1 | -- | -- | Not Used
F2 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
F3 | DK GRN/WHT | 1317 | Fog Lamp Relay Output
F4 | PPL | 34 | Fog Lamp Feed
F5-F11 | -- | -- | Not Used
F12 | GRY | 8 | IP Lamp Feed

#### RH IP Junction Block C2

Connector Part Information |

• | 12176741

• | 30-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | -- | -- | Not Used
A2 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
A3 | DK GRN | 117 | Speaker Return, Right Front
A4-A8 | -- | -- | Not Used
A9 | BRN | 9 | Parklamp Feed
A10 | -- | -- | Not Used
A11 | LT BLU | 20 | Stoplamp Feed
A12 | GRY | 8 | IP Lamp Feed
B1 | BLK/WHT | 238 | Seat Belt Switch Signal
B2 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
B3 | DK BLU | 46 | Speaker Feed, Right Rear
B4 | YEL | 116 | Speaker Return, Left Front
B5 | -- | -- | Not Used
B8 | LT BLU | 395 | Door Handle Switch Signal, Right Front
B9 | BRN | 9 | Parklamp Feed
B10 | -- | -- | Not Used
B11 | LT GRN | 24 | Backup Lamp Feed
B12 | GRY | 8 | IP Lamp Feed
C1 | LT GRN | 200 | Speaker Feed, Right Front
C2 | -- | -- | Not Used
C3 | LT BLU | 115 | Speaker Return, Right Rear
C4 | BRN | 199 | Speaker Feed, Left Front
C5 | BLK | 28 | Horn Relay Output
C8 | -- | -- | Not Used
C9 | BRN | 9 | Fuse Output, IP Lamps
C10 | BRN | 9 | Parklamp Feed
C11 | -- | -- | Not Used
C12 | GRY | 8 | IP Lamp Feed

#### RH IP Junction Block C3

Connector Part Information |

• | 12176740

• | 30-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | GRY | 8 | IP Lamp Feed
A2 | LT BLU | 20 | Stoplamp Feed
A3 | -- | -- | Not Used
A4 | BRN | 9 | Parklamp Feed
A5 | -- | -- | Not Used
A8 | BRN | 141 | Fuse Output, Ignition 3
A9 | BRN | 341 | Fuse Output, Ignition 3
A10 | DK GRN | 117 | Speaker Return, Right Front
A11 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
A12 | BRN | 541 | Fuse Output, Ignition 3
B1 | GRY | 8 | IP Lamp Feed
B2 | LT GRN | 24 | Backup Lamp Feed
B3 | -- | -- | Not Used
B4 | BRN | 9 | Parklamp Feed
B5 | LT BLU | 395 | Door Handle Switch Signal, Right Front
B8 | -- | -- | Not Used
B9 | YEL | 116 | Speaker Return, Left Front
B10 | DK BLU | 46 | Speaker Feed, Right Rear
B11 | LT BLU/BLK | 14 | Turn Signal Lamp Feed, Left Front
B12 | BLK/WHT | 238 | Seat Belt Switch Signal
C1 | GRY | 8 | IP Lamp Feed
C2 | LT GRN | 24 | Backup Lamp Feed
C3 | -- | -- | Not Used
C4 | BRN | 9 | Lamp Feed
C5 | LT BLU | 395 | Door Handle Switch Signal, Right Front
C8 | BLK | 28 | Horn Relay Output
C9 | BRN | 199 | Speaker Feed, Left Front
C10 | LT BLU | 115 | Speaker Return, Right Rear
C11 | -- | -- | Not Used
C12 | LT GRN | 200 | Speaker Feed, Right Front

#### Underhood Junction Block C1 (LD9 Only)

Connector Part Information |

• | 12161045

• | 68-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 855 | Fuse Output, ABS
A2 | DK GRN/WHT | 459 | A/C Compressor Control Relay Output
A3 | PNK | 1632 | ABS Relay Control
A4 | PNK | 1039 | Fuse Output, Ignition 1
A5 | -- | -- | Not Used
A6 | GRY | 729 | A/C Compressor Clutch Solenoid Output
A7 | -- | -- | Not Used
A8 | WHT | 121 | Tachometer Signal
A9-A10 | -- | -- | Not Used
A11 | YEL | 5 | Ignition Switch Output (CRANK)
A12 | LT BLU | 20 | Stoplamp Feed
B1 | ORN | 855 | Fuse Output, ABS
B2 | -- | -- | Not Used
B3 | RED | 1633 | ABS Relay Output
B4 | -- | -- | Not Used
B5 | PNK | 139 | Fuse Output, Ignition 1
B6 | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed
B7 | -- | -- | Not Used
B8 | BLK | 450 | Ground
B9-B12 | -- | -- | Not Used
C1-C2 | -- | -- | Not Used
C3 | DK GRN | 83 | Cruise Control Signal (Disengage)
C4-C5 | -- | -- | Not Used
C8 | PNK | 639 | Fuse Output, Ignition 1
C9 | -- | -- | Not Used
C10 | GRY | 532 | Coolant Fan Motor Feed (Secondary)
C11 | LT BLU/BLK | 396 | Cruise Control Signal (Engaged)
C12 | -- | -- | Not Used
D1-D2 | -- | -- | Not Used
D3 | DK GRN | 335 | Coolant Fan Relay Output
D4 | -- | -- | Not Used
D5 | PNK | 239 | Fuse Output, Ignition 1
D8-D9 | -- | -- | Not Used
D10 | BLK | 450 | Ground
D11 | DK BLU | 473 | Coolant Fan Relay Output (Secondary)
D12 | -- | -- | Not Used
E1 | ORN | 1640 | Fuse Output, Battery
E2 | -- | -- | Not Used
E3 | PPL | 420 | Brake Pedal Switch Output (TCC)
E4-E5 | -- | -- | Not Used
E6 | ORN | 480 | Fuse Output, Electronic Control Unit
E7 | ORN | 840 | Fuse Output, Battery
E8 | DK GRN/WHT | 465 | Fuel Pump Relay Feed
E9 | BRN | 241 | Fuse Output, Ignition 3
E10-E12 | -- | -- | Not Used
F1-F2 | -- | -- | Not Used
F3 | LT BLU | 409 | Coolant Fan Motor Feed
F4 | -- | -- | Not Used
F5 | PNK | 539 | Fuse Output, Ignition 1
F6-F8 | -- | -- | Not Used
F9 | BRN | 241 | Fuse Output, Ignition 3
F10 | -- | -- | Not Used
F11 | WHT | 504 | Coolant Fan Motor Output
F12 | -- | -- | Not Used

#### Underhood Junction Block C1 (L82 Only)

Connector Part Information |

• | 12161045

• | 68-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 855 | Fuse Output, ABS
A2 | DK GRN/WHT | 459 | A/C Compressor Control Relay Output
A3 | PNK | 1632 | ABS Relay Control
A4 | PNK | 1039 | Fuse Output, Ignition 1
A5 | -- | -- | Not Used
A6 | GRY | 729 | A/C Compressor Clutch Solenoid Output
A7 | PNK | 839 | Fuse Output, Ignition 1
A8 | WHT | 121 | Tachometer Signal
A9-A10 | -- | -- | Not Used
A11 | YEL | 5 | Ignition Switch Output (CRANK)
A12 | LT BLU | 20 | Stoplamp Feed
B1 | ORN | 855 | Fuse Output, ABS
B2 | -- | -- | Not Used
B3 | RED | 1633 | ABS Relay Output
B4 | -- | -- | Not Used
B5 | PNK | 139 | Fuse Output, Ignition 1
B6 | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed
B7 | -- | -- | Not Used
B8 | BLK | 450 | Ground
B9-B12 | -- | -- | Not Used
C1-C2 | -- | -- | Not Used
C3 | DK GRN | 83 | Cruise Control Signal (Disengage)
C4-C5 | -- | -- | Not Used
C8 | PNK | 639 | Fuse Output, Ignition 1
C9 | -- | -- | Not Used
C10 | GRY | 532 | Coolant Fan Motor Feed (Secondary)
C11 | DK BLU/BLK | 396 | Cruise Control Signal (Engaged)
C12 | -- | -- | Not Used
D1-D2 | -- | -- | Not Used
D3 | DK GRN | 335 | Coolant Fan Relay Output
D4 | -- | -- | Not Used
D5 | PNK | 239 | Fuse Output, Ignition 1
D8 | PNK | 639 | Fuse Output, Ignition 1
D9 | BRN | 241 | Fuse Output, Ignition 3
D10 | BLK | 450 | Ground
D11 | DK BLU | 473 | Coolant Fan Relay Output (Secondary)
D12 | RED/WHT | 812 | Reference Voltage Feed (12 V)
E1 | ORN | 1640 | Fuse Output, Battery
E2 | -- | -- | Not Used
E3 | PPL | 420 | Brake Pedal Switch Output (TCC)
E4-E5 | -- | -- | Not Used
E6 | ORN | 480 | Fuse Output, Electronic Control Unit
E7 | ORN | 840 | Fuse Output, Battery
E8 | DK GRN/WHT | 465 | Fuel Pump Relay Feed
E9 | BRN | 241 | Fuse Output, Ignition 3
E10 | -- | -- | Not Used
E11 | BRN | 241 | Fuse Output, Ignition 3
E12 | RED/WHT | 812 | Reference Voltage Feed (12 V)
F1-F2 | -- | -- | Not Used
F3 | LT BLU | 409 | Coolant Fan Motor Feed
F4 | -- | -- | Not Used
F5 | PNK | 539 | Fuse Output, Ignition 1
F6-F7 | -- | -- | Not Used
F8 | BRN | 241 | Fuse Output, Ignition 3
F9 | BRN | 241 | Fuse Output, Ignition 3
F10 | -- | -- | Not Used
F11 | WHT | 504 | Coolant Fan Motor Output
F12 | RED/WHT | 812 | Reference Voltage Feed (12 V)

#### Underhood Junction Block C2

Connector Part Information |

• | 12161046

• | 68-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BRN | 341 | Fuse Output, Ignition 3
A2-A3 | -- | -- | Not Used
A4 | ORN | 740 | Fuse Output, Battery
A5-A9 | -- | -- | Not Used
A10 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
A11-A12 | -- | -- | Not Used
B1-B4 | -- | -- | Not Used
B5 | BRN | 9 | Parklamp Feed
B6-B9 | -- | -- | Not Used
B10 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
B11 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
B12 | LT BLU | 20 | Stoplamp Feed
C1-C3 | -- | -- | Not Used
C4 | ORN | 740 | Fuse Output, Battery
C5 | BRN | 9 | Parklamp Feed
C8-C9 | -- | -- | Not Used
C10 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
C11 | -- | -- | Not Used
C12 | DK GRN | 29 | Horn Feed
D1-D4 | -- | -- | Not Used
D5 | BRN | 9 | Parklamp Feed
D8-D10 | -- | -- | Not Used
D11 | GRY | 589 | DRL Resistor Feed
D12 | -- | -- | Not Used
E1-E2 | -- | -- | Not Used
E3 | DK GRN | 83 | Cruise Control Signal (Disengage)
E4 | -- | -- | Not Used
E5 | BRN | 9 | Parklamp Feed
E6 | PNK | 1200 | Headlamp Lamp Output (High Beam)
E7 | -- | -- | Not Used
E8 | ORN | 640 | Fuse Output, Battery
E9 | LT BLU/BLK | 396 | Cruise Control Signal (Engaged)
E10-E11 | -- | -- | Not Used
E12 | DK BLU | 1201 | Headlamp Lamp Output (Low Beam)
F1-F3 | -- | -- | Not Used
F4 | PPL | 420 | Brake Pedal Switch Output (TCC)
F5 | -- | -- | Not Used
F6 | PNK | 1200 | Headlamp Lamp Output (High Beam)
F7 | -- | -- | Not Used
F8 | ORN | 640 | Fuse Output, Battery
F9-F11 | -- | -- | Not Used
F12 | DK BLU | 1201 | Headlamp Lamp Output (Low Beam)

#### Underhood Junction Block C3

Connector Part Information |

• | 12161047

• | 68-Way F Metri-Pack 280 Series (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 40 | Fuse Output, Battery
A2-A3 | -- | -- | Not Used
A4 | PPL | 420 | Brake Pedal Switch Output (TCC)
A5 | -- | -- | Not Used
A6 | ORN | 300 | Ignition Switch Output (Ignition 3)
A7 | BRN | 241 | Fuse Output, Ignition 3
A8-A9 | -- | -- | Not Used
A10 | BLK | 150 | Ground
A11 | BRN | 41 | Fuse Output, Ignition 3
A12 | DK BLU | 1201 | Headlamp Lamp Output (Low Beam)
B1-B2 | -- | -- | Not Used
B3 | DK GRN | 306 | Headlamp Switch Output (Headlamps OFF)
B4-B6 | -- | -- | Not Used
B7 | PNK | 1200 | Headlamp Lamp Output (High Beam)
B8 | WHT | 1080 | Parklamp Relay Output
B9 | PPL | 65 | Blower Motor Feed
B10-B11 | -- | -- | Not Used
B12 | LT GRN/BLK | 592 | DRL Relay Output
C1-C3 | -- | -- | Not Used
C4 | PNK | 439 | Fuse Output, Ignition 1
C5 | PPL | 293 | Rear Defogger Element Feed
C8 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
C9 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
C10 | DK BLU | 101 | Blower Resistor Output
C11 | PNK/WHT | 1970 | Headlamp Relay Output (Low Beam)
C12 | BLK | 28 | Horn Relay Output
D1 | -- | -- | Not Used
D2 | BRN | 341 | Fuse Output, Ignition 3
D3-D4 | -- | -- | Not Used
D5 | WHT | 193 | Rear Defogger Relay Output
D8 | ORN | 240 | Fuse Output, Battery
D9 | ORN | 52 | Blower Switch Output (HIGH)
D10-D12 | -- | -- | Not Used
E1-E5 | -- | -- | Not Used
E6 | GRY | 120 | Fuel Pump Motor Feed
E7-E12 | -- | -- | Not Used
F1-F4 | -- | -- | Not Used
F5 | PNK | 3 | Ignition Switch Output (Ignition 1)
F6 | -- | -- | Not Used
F7 | BRN | 9 | Parklamp Feed
F8 | WHT | 121 | Tachometer Signal
F9-F10 | -- | -- | Not Used
F11 | YEL | 5 | Ignition Switch Output (CRANK)
F12 | LT BLU | 20 | Stoplamp Feed

#### Underhood Junction Block C4

Connector Part Information |

• | 12146038

• | 2-Way F Metri-Pack 800 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 842 | Fuse Output, Battery
B | RED | 242 | Fuse Output, Battery

#### Underhood Junction Block C5

Connector Part Information |

• | 12160605

• | 2-Way F Metri-Pack 800 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RED | 442 | Fuse Output, Battery

#### Underhood Junction Block C6

Connector Part Information |

• | 12146037

• | 2-Way F Metri-Pack 800 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RED | 642 | Fuse Output, Battery

#### Underhood Junction Block C7

Connector Part Information |

• | 12160606

• | 2-Way F Metri-Pack 800 Series (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RED | 1042 | Fuse Output, Battery