For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the left front wheel. Refer to Tires and Wheels in Suspension.
3. Remove the mount thru bolt.
4. Remove the mount bolts.
5. Remove the mount out the left wheel opening.

### Installation Procedure

1. Install the mount.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the mount bolts.

Tighten
Tighten the bolts to 122 N·m (90 lb ft).

3. Install the mount thru bolt.

Tighten
Tighten the bolts to 120 N·m (89 lb ft).

4. Install the left front wheel. Refer to Tires and Wheels in Suspension.
5. Lower the vehicle.