For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 41239-2 Cooler Pipe Seal Remover

• | J 6125-1B Slide Hammer

• | J 6471 Slide Hammer Adapter

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the transmission oil cooler lines from the transmission.
3. Install the J 41239-2 into the cooler line seal.
4. Remove the oil cooler line seals (49). Use the J 41239-2 .

### Installation Procedure

#### Tools Required

J 41239-1A Cooler Pipe Seal Installer

1. Use DEXRON III, or equivalent, Automatic Transmission Fluid in order to lube the seal and the transaxle bores thoroughly.
2. Install the J 41239-1A on the transmission case using cooler line bracket bolt.
3. Install a new seal in the case bore.
4. Press the new seals in. Tighten the cooler line bracket bolt until the seal bottoms out in the case bore.
5. Install the transmission oil cooler lines.
6. Lower the vehicle.
7. Check the fluid level.