For 1990-2009 cars

### Removal Procedure

1. Relieve fuel system pressure. Refer to Fuel Pressure Relief Procedure .
2. Drain the fuel tank. Refer to Fuel Tank Draining Procedure .
3. Remove the fuel tank. Refer to Fuel Tank Replacement .
4. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
5. Note the strainer position for future reference.
6. Support the reservoir with one hand and grasp the strainer with the other hand.
7. Use a screwdriver to pry the strainer ferrule off the reservoir.
8. Discard the strainer.

### Installation Procedure

1. Install the new strainer (1) to reservoir.
2. Support the reservoir with one hand and grasp the strainer with the other hand twisting the strainer into position.
3. Install the fuel sender assembly. Refer toFuel Sender Assembly Replacement
4. Install the fuel tank. Refer toFuel Tank Replacement
5. Refill tank.
6. Inspect for fuel leaks:

6.1. | Turn the ignition switch to the ON position for two seconds.

6.2. | Turn the ignition switch OFF position for ten seconds.

6.3. | Turn the ignition switch to the ON position.

6.4. | Check for fuel leaks.