For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the hood latch. Refer to Hood Primary and Secondary Latch Replacement .
3. Remove the hood latch support nuts (2).
4. Remove the hood latch support bolts (1).
5. Remove the hood latch support (3).

### Installation Procedure

1. Install the hood latch support (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the hood latch support bolts (1).

Tighten
Tighten the bolts to 9 N·m (80 lb in).

3. Install the hood latch support nuts (2).

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

4. Install the hood latch. Refer to Hood Primary and Secondary Latch Replacement .